## Phidget LCD.lvlib:LCDSetContrast.vi

Contrast level of the text or graphic pixels.

- A higher contrast will make the image darker.
- `Contrast` is bounded by `MinContrast` and `MaxContrast`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Contrast The contrast value 1202_0 (ver: 100) Text LCD: Min: 0 Max: 1 Def: 0.6 1202_0 (ver: 120, 121) Text LCD: Min: 0 Max: 1 Def: 0.6 1202_1 (ver: 123, 124) Text LCD: Min: 0 Max: 1 Def: 0.6 1203_0 (ver: 100) Text LCD: Min: 0 Max: 1 Def: 0.6 1203_0 (ver: 120, 121) Text LCD: Min: 0 Max: 1 Def: 0.6 1203_1 (ver: 123, 124) Text LCD: Min: 0 Max: 1 Def: 0.6 1202_2 (ver: 200, 201, 202, 203, 204) Text LCD: Min: 0 Max: 1 Def: 0.6 1203_2 (ver: 200, 201, 202, 203, 204) Text LCD: Min: 0 Max: 1 Def: 0.6 1204_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1 1215_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1 Def: 0.6 1216_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1 Def: 0.6 1217_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1 Def: 0.6 1218_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1 Def: 0.6 1219_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1 1220_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1 1221_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1 1222_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1 LCD1100_0 (ver: 100) Graphic LCD: Min: 0 Max: 1 Def: 0.25

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.