## Phidget Temperature Sensor.lvlib:TemperatureGetMinDataInterval.vi

The minimum value that `DataInterval` can be set to.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Min Data Interval The data interval value Units: milliseconds (ms) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Val: 32 1045_1 (ver: 101) Temperature Sensor (IR): Val: 32 1045_0 (ver: 100, 101) Temperature Sensor (IC): Val: 32 1045_1 (ver: 101) Temperature Sensor (IC): Val: 32 1048_0 (ver: 100, 101, 102) Thermocouple Input: Val: 32 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Val: 32 1051_0 (ver: 100) Thermocouple Input: Val: 32 1051_0 (ver: 100) Temperature Sensor (IC): Val: 32 1051_0 (ver: 200, 201, 202) Thermocouple Input: Val: 32 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Val: 32 1051_1 (ver: 300) Thermocouple Input: Val: 32 1051_1 (ver: 300) Temperature Sensor (IC): Val: 32 1051_2 (ver: 400, 401, 402) Thermocouple Input: Val: 32 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Val: 32 DCC1000_0 (ver: 100) Temperature Sensor: Val: 500 HUM1000_0 (ver: 100) Temperature Sensor: Val: 500 SAF1000_0 (ver: 100) Temperature Sensor: Val: 100 TMP1000_0 (ver: 100) Temperature Sensor (IC): Val: 500 TMP1100_0 (ver: 100) Thermocouple Input: Val: 20 TMP1100_0 (ver: 100) Temperature Sensor (IC): Val: 300 TMP1101_0 (ver: 100) Thermocouple Input: Val: 20 TMP1101_0 (ver: 100) Temperature Sensor (IC): Val: 300 TMP1200_0 (ver: 100) RTD input: Val: 250 TMP1300_0 (ver: 100) Temperature Sensor (IR): Val: 20 TMP1300_0 (ver: 100) Temperature Sensor (IC): Val: 20