## Phidget Encoder.lvlib:EncoderGetPosition.vi

The most recent position value that the controller has reported.

- Position counts either quadrature pulses or quadrature cycles. See your controller's User Guide for more information.
- When you set Position to a certain value, it is set per-channel rather than per-device, so other users who have the same channel open will not see the change.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Position The position value 1047_0 (ver: 100, 101, 102) Encoder Input: Val: 0 1047_1 (ver: 102, 103) Encoder Input: Val: 0 1052_0 (ver: 100) Encoder Input: Val: 0 1052_0 (ver: 101, 102, 103) Encoder Input: Val: 0 1052_0 (ver: 110, 111) Encoder Input: Val: 0 1057_0 (ver: 300, 301) Encoder Input: Val: 0 1057_1 (ver: 302) Encoder Input: Val: 0 1057_2 (ver: 302) Encoder Input: Val: 0 1065_0 (ver: 100, 101) Encoder Input: Val: 0 DCC1000_0 (ver: 100) Encoder Input: Val: 0 ENC1000_0 (ver: 100) Encoder Input: Val: 0