## Phidget RFID.lvlib:RFIDGetTagPresent.vi

This property is true if a compatibile RFID tag is being read by the reader.

- `TagPresent` will remain true until the tag is out of range and can no longer be read.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Tag Present Tag is in range 1023_0 (ver: 103) RFID Reader: 1023_0 (ver: 104) RFID Reader: 1023_0 (ver: 200) RFID Reader: 1023_0 (ver: 201, 202, 203, 204) RFID Reader: 1023_1 (ver: 205, 206) RFID Reader: 1024_0 (ver: 100, 101) RFID Reader/Writer: