## Phidget Voltage Ratio Input.lvlib:VoltageRatioInputStart.vi

Opens and initializes a Phidget Voltage Ratio Input

| Change Trigger The change trigger value Units: volts/volt (V/V) 1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1013_0 (ver: 821, 823) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1018_1 (ver: 826) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1019_0 (ver: 826) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1070_0 (ver: 826) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1010_0 (ver: 903, 904) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1019_1 (ver: 903, 904) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1072_0 (ver: 903) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1073_0 (ver: 904) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1046_0 (ver: 100, 101) Bridge Input: Min: 0 Max: 1 Def: 0 1046_0 (ver: 102) Bridge Input: Min: 0 Max: 1 Def: 0 1065_0 (ver: 100, 101) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1202_0 (ver: 100) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1203_0 (ver: 100) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1202_0 (ver: 120, 121) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1202_1 (ver: 123, 124) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1203_0 (ver: 120, 121) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1203_1 (ver: 123, 124) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 HUB0000_0 (ver: 115) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 SBC3003_0 (ver: 100) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 DAQ1000_0 (ver: 100) Voltage Ratio Input: Min: 0 Max: 1 Def: 0 DAQ1500_0 (ver: 100) Bridge Input: Min: 0 Max: 0.5 Def: 0 DCC1000_0 (ver: 100) Voltage Ratio: Min: 0 Max: 1Val: 0 HIN1100_0 (ver: 100) Joystick Axis: Min: 0 Max: 2 Def: 0

| Data Interval The data interval for the channel Units: milliseconds (ms) 1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1013_0 (ver: 821, 823) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1018_1 (ver: 826) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1019_0 (ver: 826) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1070_0 (ver: 826) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1010_0 (ver: 903, 904) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1019_1 (ver: 903, 904) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1072_0 (ver: 903) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1073_0 (ver: 904) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1046_0 (ver: 100, 101) Bridge Input: Min: 8 Max: 1000 Def: 256 1046_0 (ver: 102) Bridge Input: Min: 8 Max: 1000 Def: 256 1065_0 (ver: 100, 101) Voltage Ratio Input: Min: 8 Max: 60000 Def: 256 1202_0 (ver: 100) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1203_0 (ver: 100) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1202_0 (ver: 120, 121) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1202_1 (ver: 123, 124) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1203_0 (ver: 120, 121) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1203_1 (ver: 123, 124) Voltage Ratio Input: Min: 16 Max: 1000 Def: 256 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Min: 1 Max: 1000 Def: 256 HUB0000_0 (ver: 115) Voltage Ratio Input: Min: 1 Max: 60000 Def: 250 SBC3003_0 (ver: 100) Voltage Ratio Input: Min: 1 Max: 60000 Def: 250 DAQ1000_0 (ver: 100) Voltage Ratio Input: Min: 20 Max: 60000 Def: 250 DAQ1500_0 (ver: 100) Bridge Input: Min: 20 Max: 60000 Def: 250 DCC1000_0 (ver: 100) Voltage Ratio: Min: 100 Max: 60000Val: 250 HIN1100_0 (ver: 100) Joystick Axis: Min: 20 Max: 1000 Def: 100

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| IsHubPort The hub port mode

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Bridge Gain The bridge gain value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1046_0 v100 v101 | 1046_0 v102 | DAQ1500_0 v100
BRIDGE_GAIN_1 | 1 | ✓ | ✓ | ✓
BRIDGE_GAIN_2 | 2 | X | X | ✓
BRIDGE_GAIN_4 | 3 | X | X | X
BRIDGE_GAIN_8 | 4 | ✓ | ✓ | X
BRIDGE_GAIN_16 | 5 | ✓ | ✓ | X
BRIDGE_GAIN_32 | 6 | ✓ | ✓ | X
BRIDGE_GAIN_64 | 7 | ✓ | ✓ | ✓
BRIDGE_GAIN_128 | 8 | ✓ | ✓ | ✓
1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Unsupported 1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Unsupported 1013_0 (ver: 821, 823) Voltage Ratio Input: Unsupported 1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Unsupported 1018_1 (ver: 826) Voltage Ratio Input: Unsupported 1019_0 (ver: 826) Voltage Ratio Input: Unsupported 1070_0 (ver: 826) Voltage Ratio Input: Unsupported 1010_0 (ver: 903, 904) Voltage Ratio Input: Unsupported 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Unsupported 1019_1 (ver: 903, 904) Voltage Ratio Input: Unsupported 1072_0 (ver: 903) Voltage Ratio Input: Unsupported 1073_0 (ver: 904) Voltage Ratio Input: Unsupported 1046_0 (ver: 100, 101) Bridge Input: Def: BRIDGE_GAIN_128 1046_0 (ver: 102) Bridge Input: Def: BRIDGE_GAIN_128 1065_0 (ver: 100, 101) Voltage Ratio Input: Unsupported 1202_0 (ver: 100) Voltage Ratio Input: Unsupported 1203_0 (ver: 100) Voltage Ratio Input: Unsupported 1202_0 (ver: 120, 121) Voltage Ratio Input: Unsupported 1202_1 (ver: 123, 124) Voltage Ratio Input: Unsupported 1203_0 (ver: 120, 121) Voltage Ratio Input: Unsupported 1203_1 (ver: 123, 124) Voltage Ratio Input: Unsupported 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Unsupported 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Unsupported HUB0000_0 (ver: 115) Voltage Ratio Input: Unsupported SBC3003_0 (ver: 100) Voltage Ratio Input: Unsupported DAQ1000_0 (ver: 100) Voltage Ratio Input: Unsupported DAQ1500_0 (ver: 100) Bridge Input: Def: BRIDGE_GAIN_128 DCC1000_0 (ver: 100) Voltage Ratio: Unsupported HIN1100_0 (ver: 100) Joystick Axis: Unsupported

| Bridge Enabled The enabled value 1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Unsupported 1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Unsupported 1013_0 (ver: 821, 823) Voltage Ratio Input: Unsupported 1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Unsupported 1018_1 (ver: 826) Voltage Ratio Input: Unsupported 1019_0 (ver: 826) Voltage Ratio Input: Unsupported 1070_0 (ver: 826) Voltage Ratio Input: Unsupported 1010_0 (ver: 903, 904) Voltage Ratio Input: Unsupported 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Unsupported 1019_1 (ver: 903, 904) Voltage Ratio Input: Unsupported 1072_0 (ver: 903) Voltage Ratio Input: Unsupported 1073_0 (ver: 904) Voltage Ratio Input: Unsupported 1046_0 (ver: 100, 101) Bridge Input: Val: 0 1046_0 (ver: 102) Bridge Input: Val: 0 1065_0 (ver: 100, 101) Voltage Ratio Input: Unsupported 1202_0 (ver: 100) Voltage Ratio Input: Unsupported 1203_0 (ver: 100) Voltage Ratio Input: Unsupported 1202_0 (ver: 120, 121) Voltage Ratio Input: Unsupported 1202_1 (ver: 123, 124) Voltage Ratio Input: Unsupported 1203_0 (ver: 120, 121) Voltage Ratio Input: Unsupported 1203_1 (ver: 123, 124) Voltage Ratio Input: Unsupported 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Unsupported 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Unsupported HUB0000_0 (ver: 115) Voltage Ratio Input: Unsupported SBC3003_0 (ver: 100) Voltage Ratio Input: Unsupported DAQ1000_0 (ver: 100) Voltage Ratio Input: Unsupported DAQ1500_0 (ver: 100) Bridge Input: Def: 1 DCC1000_0 (ver: 100) Voltage Ratio: Unsupported HIN1100_0 (ver: 100) Joystick Axis: Unsupported

| Sensor Type The sensor type value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
| 1011_0 v100 v101 v102 v103 | 1013_0 v800 v811 v820 | 1013_0 v821 v823 | 1018_0 v824 v825 v826 | 1018_1 v826 | 1019_0 v826 | 1070_0 v826 | 1010_0 v903 v904 | 1018_2 v900 v901 v902 v903 v904 | 1019_1 v903 v904 | 1072_0 v903 | 1073_0 v904 | 1065_0 v100 v101 | 1202_0 v100 | 1203_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | HUB0000_0 v115 | SBC3003_0 v100 | DAQ1000_0 v100 | DCC1000_0 v100 | HIN1100_0 v100
SENSOR_TYPE_VOLTAGERATIO | 0 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
SENSOR_TYPE_1101_SHARP_2D120X | 11011 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1101_SHARP_2Y0A21 | 11012 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1101_SHARP_2Y0A02 | 11013 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1102 | 11020 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1103 | 11030 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1104 | 11040 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1105 | 11050 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1106 | 11060 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1107 | 11070 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1108 | 11080 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1109 | 11090 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1110 | 11100 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1111 | 11110 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1112 | 11120 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1113 | 11130 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1115 | 11150 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1116 | 11160 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1118_AC | 11181 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1118_DC | 11182 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1119_AC | 11191 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1119_DC | 11192 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1120 | 11200 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1121 | 11210 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1122_AC | 11221 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1122_DC | 11222 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1124 | 11240 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1125_HUMIDITY | 11251 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1125_TEMPERATURE | 11252 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1126 | 11260 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1128 | 11280 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1129 | 11290 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1131 | 11310 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1134 | 11340 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1136 | 11360 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1137 | 11370 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1138 | 11380 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1139 | 11390 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1140 | 11400 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1141 | 11410 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_1146 | 11460 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3120 | 31200 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3121 | 31210 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3122 | 31220 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3123 | 31230 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3130 | 31300 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3520 | 35200 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3521 | 35210 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SENSOR_TYPE_3522 | 35220 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X

1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1013_0 (ver: 821, 823) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1018_1 (ver: 826) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1019_0 (ver: 826) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1070_0 (ver: 826) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1010_0 (ver: 903, 904) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1019_1 (ver: 903, 904) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1072_0 (ver: 903) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1073_0 (ver: 904) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1046_0 (ver: 100, 101) Bridge Input: Unsupported

1046_0 (ver: 102) Bridge Input: Unsupported

1065_0 (ver: 100, 101) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1202_0 (ver: 100) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1203_0 (ver: 100) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1202_0 (ver: 120, 121) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1202_1 (ver: 123, 124) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1203_0 (ver: 120, 121) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1203_1 (ver: 123, 124) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

HUB0000_0 (ver: 115) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

SBC3003_0 (ver: 100) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

DAQ1000_0 (ver: 100) Voltage Ratio Input: Def: SENSOR_TYPE_VOLTAGERATIO

DAQ1500_0 (ver: 100) Bridge Input: Unsupported

DCC1000_0 (ver: 100) Voltage Ratio: Def: SENSOR_TYPE_VOLTAGERATIO

HIN1100_0 (ver: 100) Joystick Axis: Val: SENSOR_TYPE_VOLTAGERATIO

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number