## Phidget Magnetometer.lvlib:MagnetometerGetAxisCount.vi

The number of axes the controller can measure field strength on.

- See your controller's User Guide for more information about the number of axes and their orientation.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Axis Count The axis count value 1042_0 (ver: 300, 301, 302) 3-Axis Magnetometer: Val: 3 1044_0 (ver: 400, 401, 402) 3-Axis Magnetometer: Val: 3 1056_0 (ver: 100, 101, 102) 3-Axis Magnetometer: Val: 3 1056_0 (ver: 200) 3-Axis Magnetometer: Val: 3 MOT1101_0 (ver: 100) 3-Axis Magnetometer: Val: 3