## Phidget Voltage Input.lvlib:VoltageInputGetSensorValue.vi

The most recent sensor value that the controller has reported.

- Use `SensorUnit` to get the measurement units that are associated with the `SensorValue`

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Sensor Value The sensor value 1011_0 (ver: 100, 101, 102, 103) Voltage Input: 1013_0 (ver: 800, 811, 820) Voltage Input: 1013_0 (ver: 821, 823) Voltage Input: 1018_0 (ver: 824, 825, 826) Voltage Input: 1018_1 (ver: 826) Voltage Input: 1019_0 (ver: 826) Voltage Input: 1070_0 (ver: 826) Voltage Input: 1010_0 (ver: 903, 904) Voltage Input: 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: 1019_1 (ver: 903, 904) Voltage Input: 1072_0 (ver: 903) Voltage Input: 1073_0 (ver: 904) Voltage Input: 1048_0 (ver: 100, 101, 102) Voltage Input: Unsupported 1051_0 (ver: 200, 201, 202) Voltage Input: Unsupported 1051_1 (ver: 300) Voltage Input: Unsupported 1051_2 (ver: 400, 401, 402) Voltage Input: Unsupported 1058_0 (ver: 100, 101) Voltage Input: Unsupported 1065_0 (ver: 100, 101) Voltage Input: 1065_0 (ver: 100, 101) Supply Voltage Sensor: Unsupported 1202_0 (ver: 100) Voltage Input: 1203_0 (ver: 100) Voltage Input: 1202_0 (ver: 120, 121) Voltage Input: 1202_1 (ver: 123, 124) Voltage Input: 1203_0 (ver: 120, 121) Voltage Input: 1203_1 (ver: 123, 124) Voltage Input: 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: HUB0000_0 (ver: 115) Voltage Input: SBC3003_0 (ver: 100) Voltage Input: ADP1000_0 (ver: 100) Voltage Input: DAQ1000_0 (ver: 100) Voltage Input: DAQ1400_0 (ver: 100) Voltage Input: Unsupported SAF1000_0 (ver: 100) Voltage Sensor: Unsupported TMP1100_0 (ver: 100) Voltage Input: Unsupported TMP1101_0 (ver: 100) Voltage Input: Unsupported TMP1300_0 (ver: 100) Voltage Input: Unsupported VCP1000_0 (ver: 100) Voltage Input: Unsupported VCP1001_0 (ver: 100) Voltage Input: Unsupported VCP1002_0 (ver: 100) Voltage Input: Unsupported