## Phidget Temperature Sensor.lvlib:TemperatureEventExe.vi

The most recent temperature value the controller has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

- If a `TemperatureChangeTrigger` has been set to a non-zero value, the `TemperatureChange` event will not occur until the temperature has changed by at least the `TemperatureChangeTrigger` value.

Device Support:

1045_0 (ver: 100, 101) Temperature Sensor (IR) : Supported

1045_1 (ver: 101) Temperature Sensor (IR) : Supported

1045_0 (ver: 100, 101) Temperature Sensor (IC) : Supported

1045_1 (ver: 101) Temperature Sensor (IC) : Supported

1048_0 (ver: 100, 101, 102) Thermocouple Input : Supported

1048_0 (ver: 100, 101, 102) Temperature Sensor (IC) : Supported

1051_0 (ver: 100) Thermocouple Input : Supported

1051_0 (ver: 100) Temperature Sensor (IC) : Supported

1051_0 (ver: 200, 201, 202) Thermocouple Input : Supported

1051_0 (ver: 200, 201, 202) Temperature Sensor (IC) : Supported

1051_1 (ver: 300) Thermocouple Input : Supported

1051_1 (ver: 300) Temperature Sensor (IC) : Supported

1051_2 (ver: 400, 401, 402) Thermocouple Input : Supported

1051_2 (ver: 400, 401, 402) Temperature Sensor (IC) : Supported

DCC1000_0 (ver: 100) Temperature Sensor : Supported

HUM1000_0 (ver: 100) Temperature Sensor : Supported

SAF1000_0 (ver: 100) Temperature Sensor : Supported

TMP1000_0 (ver: 100) Temperature Sensor (IC) : Supported

TMP1100_0 (ver: 100) Thermocouple Input : Supported

TMP1100_0 (ver: 100) Temperature Sensor (IC) : Supported

TMP1101_0 (ver: 100) Thermocouple Input : Supported

TMP1101_0 (ver: 100) Temperature Sensor (IC) : Supported

TMP1200_0 (ver: 100) RTD input : Supported

TMP1300_0 (ver: 100) Temperature Sensor (IR) : Supported

TMP1300_0 (ver: 100) Temperature Sensor (IC) : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| Temperature The temperature

| Event Registration Refnum Out Same as Event Registration Refnum In