## Phidget DC Motor.lvlib:DCMotorSetTargetBrakingStrength.vi

When a motor is not being actively driven forward or reverse, you can choose if the motor will be allowed to freely turn, or will resist being turned.

- A low `TargetBrakingStrength` value corresponds to free wheeling, this will have the following effects:
  - The motor will continue to rotate after the controller is no longer driving the motor (i.e. `Velocity` is 0), due to inertia.
  - The motor shaft will provide little resistance to being turned when it is stopped.
- A higher `TargetBrakingStrength` value will resist being turned, this will have the following effects:
  - The motor will more stop more quickly if it is in motion and braking has been requested. It will fight against the rotation of the shaft.
- Braking mode is enabled by setting the `Velocity` to `MinVelocity`

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Target Braking Strength The braking value 1060_0 (ver: 100, 110) DC Motor Controller: Val: 0 1064_0 (ver: 100, 101, 102) DC Motor Controller: Val: 0 1064_1 (ver: 102) DC Motor Controller: Val: 0 1065_0 (ver: 100, 101) DC Motor Controller: Def: 0 DCC1000_0 (ver: 100) DC Motor Controller: Val: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.