## Phidget Accelerometer.lvlib:AccelerometerGetAcceleration.vi

The most recent acceleration value that the controller has reported.

- This value will always be between `MinAcceleration` and `MaxAcceleration`.

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device In Device # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| Acceleration The acceleration values Units: g-force (g) 1008_0 (ver: 101) 2-Axis Accelerometer: Min: -2 Max: 2 1041_0 (ver: 200, 201, 202) 3-Axis Accelerometer: Min: -8 Max: 8 1042_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: -8 Max: 8 1043_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: -8 Max: 8 1044_0 (ver: 400, 401, 402) 3-Axis Accelerometer: Min: -8 Max: 8 1049_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: -5 Max: 5 1053_0 (ver: 300, 301, 302) 2-Axis Accelerometer: Min: -5 Max: 5 1056_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: -5 Max: 5 1056_0 (ver: 200) 3-Axis Accelerometer: Min: -5 Max: 5 1059_0 (ver: 400, 401) 3-Axis Accelerometer: Min: -3 Max: 3 MOT1100_0 (ver: 100) 3-Axis Accelerometer: Min: -8 Max: 8 MOT1101_0 (ver: 100) 3-Axis Accelerometer: Min: -8 Max: 8

| Acceleration Acceleraiton on the indexed axis.