## Phidget Temperature Sensor.lvlib:TemperatureSetDataInterval.vi

The `DataInterval` is the time that must elapse before the controller will fire another `TemperatureChange` event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.
- The timing between `TemperatureChange` events can also affected by the `TemperatureChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Min: 32 Max: 60000 Def: 256 1045_1 (ver: 101) Temperature Sensor (IR): Min: 32 Max: 60000 Def: 256 1045_0 (ver: 100, 101) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1045_1 (ver: 101) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_0 (ver: 100, 101, 102) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_0 (ver: 100) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 100) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 DCC1000_0 (ver: 100) Temperature Sensor: Min: 500 Max: 60000Val: 500 HUM1000_0 (ver: 100) Temperature Sensor: Min: 500 Max: 60000 Def: 500 SAF1000_0 (ver: 100) Temperature Sensor: Min: 100 Max: 60000 Def: 250 TMP1000_0 (ver: 100) Temperature Sensor (IC): Min: 500 Max: 60000Val: 500 TMP1100_0 (ver: 100) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1100_0 (ver: 100) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1101_0 (ver: 100) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1101_0 (ver: 100) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1200_0 (ver: 100) RTD input: Min: 250 Max: 60000 Def: 250 TMP1300_0 (ver: 100) Temperature Sensor (IR): Min: 20 Max: 60000 Def: 250 TMP1300_0 (ver: 100) Temperature Sensor (IC): Min: 20 Max: 60000 Def: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.