## Phidget Encoder.lvlib:EncoderSetTrigger.vi

The controller will not issue a `PositionChange` event until the position value has changed by the amount specified by the `PositionChangeTrigger`.

- Setting the `PositionChangeTrigger` to 0 will result in the controller firing events every `DataInterval`. This is useful for applications that implement their own data filtering

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Trigger The change trigger value 1047_0 (ver: 100, 101, 102) Encoder Input: Min: 0 Max: 10000 Def: 0 1047_1 (ver: 102, 103) Encoder Input: Min: 0 Max: 10000 Def: 0 1052_0 (ver: 100) Encoder Input: Min: 0 Max: 10000 Def: 0 1052_0 (ver: 101, 102, 103) Encoder Input: Min: 0 Max: 10000 Def: 0 1052_0 (ver: 110, 111) Encoder Input: Min: 0 Max: 10000 Def: 0 1057_0 (ver: 300, 301) Encoder Input: Min: 0 Max: 10000 Def: 0 1057_1 (ver: 302) Encoder Input: Min: 0 Max: 10000 Def: 0 1057_2 (ver: 302) Encoder Input: Min: 0 Max: 10000 Def: 0 1065_0 (ver: 100, 101) Encoder Input: Min: 0 Max: 10000 Def: 0 DCC1000_0 (ver: 100) Encoder Input: Min: 0 Max: 60000000Val: 0 ENC1000_0 (ver: 100) Encoder Input: Min: 0 Max: 60000000 Def: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.