## Phidget Sound Sensor.lvlib:SoundSensorGetOctaves.vi

The unweighted value of each frequency band.

- The following frequency bands are represented:

- octaves[0] = 31.5 Hz
- octaves[1] = 63 Hz
- octaves[2] = 125 Hz
- octaves[3] = 250 Hz
- octaves[4] = 500 Hz
- octaves[5] = 1 kHz
- octaves[6] = 2 kHz
- octaves[7] = 4 kHz
- octaves[8] = 8 kHz
- octaves[9] = 16 kHz

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Octaves The octave values Units: sound pressure level (dB SPL) SND1000_0 (ver: 100) Sound Sensor:

| Octave Octave