## Phidget Current Input.lvlib:CurrentInputEventExe.vi

The most recent current value the controller has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

- If a `CurrentChangeTrigger` has been set to a non-zero value, the `CurrentChange` event will not occur until the current value has changed by at least the `CurrentChangeTrigger` value.

Device Support:

1061_0 (ver: 100) RC Servo Motor Current Sensor : Supported

1061_0 (ver: 200) RC Servo Motor Current Sensor : Supported

1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Current Sensor : Supported

1063_0 (ver: 100) Bipolar Stepper Current Sensor : Supported

1063_1 (ver: 100, 101) Bipolar Stepper Current Sensor : Supported

1064_0 (ver: 100, 101, 102) DC Motor Current Sensor : Supported

1064_1 (ver: 102) DC Motor Current Sensor : Supported

1065_0 (ver: 100, 101) DC Motor Current Sensor : Supported

1066_0 (ver: 100) RC Servo Motor Current Sensor : Supported

1066_1 (ver: 100, 101) RC Servo Motor Current Sensor : Supported

DAQ1400_0 (ver: 100) Current Input : Supported

DCC1000_0 (ver: 100) Current Sensor : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| Current The current value

| phid Device # Identification of the device that triggered the event.

| Event Registration Refnum Out Same as Event Registration Refnum In