## Phidget Temperature Sensor.lvlib:TemperatureSetTrigger.vi

The controller will not issue a `TemperatureChange` event until the temperature value has changed by the amount specified by the `TemperatureChangeTrigger`.

- Setting the `TemperatureChangeTrigger` to 0 will result in the controller firing events every `DataInterval`. This is useful for applications that implement their own data filtering

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Trigger The change trigger value Units: degrees celsius (°C) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Min: 0 Max: 1000 Def: 0 1045_1 (ver: 101) Temperature Sensor (IR): Min: 0 Max: 1000 Def: 0 1045_0 (ver: 100, 101) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1045_1 (ver: 101) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1048_0 (ver: 100, 101, 102) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_0 (ver: 100) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_0 (ver: 100) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_0 (ver: 200, 201, 202) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_1 (ver: 300) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_1 (ver: 300) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_2 (ver: 400, 401, 402) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 DCC1000_0 (ver: 100) Temperature Sensor: Min: 0 Max: 165Val: 0 HUM1000_0 (ver: 100) Temperature Sensor: Min: 0 Max: 125 Def: 0 SAF1000_0 (ver: 100) Temperature Sensor: Min: 0 Max: 165 Def: 0 TMP1000_0 (ver: 100) Temperature Sensor (IC): Min: 0 Max: 125Val: 0 TMP1100_0 (ver: 100) Thermocouple Input: Min: 0 Max: 1640 Def: 0 TMP1100_0 (ver: 100) Temperature Sensor (IC): Min: 0 Max: 125 Def: 0 TMP1101_0 (ver: 100) Thermocouple Input: Min: 0 Max: 1640 Def: 0 TMP1101_0 (ver: 100) Temperature Sensor (IC): Min: 0 Max: 125 Def: 0 TMP1200_0 (ver: 100) RTD input: Min: 0 Max: 1050 Def: 0 TMP1300_0 (ver: 100) Temperature Sensor (IR): Min: 0 Max: 100 Def: 0 TMP1300_0 (ver: 100) Temperature Sensor (IC): Min: 0 Max: 500 Def: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.