## Phidget LCD.lvlib:LCDCopy.vi

Copies all pixels from a specified rectangular region to another.

Device Support:

1202_0 (ver: 100) Text LCD : Unsupported

1202_0 (ver: 120, 121) Text LCD : Unsupported

1202_1 (ver: 123, 124) Text LCD : Unsupported

1203_0 (ver: 100) Text LCD : Unsupported

1203_0 (ver: 120, 121) Text LCD : Unsupported

1203_1 (ver: 123, 124) Text LCD : Unsupported

1202_2 (ver: 200, 201, 202, 203, 204) Text LCD : Unsupported

1203_2 (ver: 200, 201, 202, 203, 204) Text LCD : Unsupported

1204_0 (ver: 100, 101) Text LCD : Unsupported

1215_0 (ver: 100, 101) Text LCD : Unsupported

1216_0 (ver: 100, 101) Text LCD : Unsupported

1217_0 (ver: 100, 101) Text LCD : Unsupported

1218_0 (ver: 100, 101) Text LCD : Unsupported

1219_0 (ver: 110, 111, 113) Text LCD : Unsupported

1220_0 (ver: 110, 111, 113) Text LCD : Unsupported

1221_0 (ver: 110, 111, 113) Text LCD : Unsupported

1222_0 (ver: 110, 111, 113) Text LCD : Unsupported

LCD1100_0 (ver: 106, 107) Graphic LCD : Supported

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| srcFramebuffer ${Copy:srcFramebuffer}

| dstFramebuffer ${Copy:dstFramebuffer}

| srcX1 ${Copy:srcX1}

| srcY1 ${Copy:srcY1}

| srcY2 ${Copy:srcY2}

| srcX2 ${Copy:srcX2}

| dstX ${Copy:dstX}

| dstY ${Copy:dstY}

| inverted If true, copied pixels are inverted

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.