## Phidget Stepper.lvlib:StepperSetCurrentLimit.vi

The current through the motor will be limited by the `CurrentLimit`.

- See your Stepper motor's data sheet for more information about what value the `CurrentLimit` should be.

  | Device In Device # Identification

  | error in (no error) error in can accept error information wired from VIs previously called.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | Current Limit The current limit value Units: amperes (A) 1062_0 (ver: 101) Unipolar Stepper Controller: Unsupported 1062_1 (ver: 101, 102) Unipolar Stepper Controller: Unsupported 1063_0 (ver: 100) Bipolar Stepper Controller: Min: 0.0542 Max: 2.492 Def: 1 1063_1 (ver: 100, 101) Bipolar Stepper Controller: Min: 0.0542 Max: 2.492 Def: 1 1067_0 (ver: 200, 201) Bipolar Stepper Controller: Min: 0 Max: 4 Def: 1 STC1000_0 (ver: 100) Bipolar Stepper Controller: Min: 0 Max: 4 Def: 1 STC1001_0 (ver: 100) Bipolar Stepper Controller: Min: 0 Max: 2.5 Def: 1 STC1002_0 (ver: 101) Bipolar Stepper Controller: Min: 0 Max: 8 Def: 1

  | Device Out Same as Device In

  | error out error out passes error or warning information out of a VI to be used by other VIs.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.