## Phidget RC Servo.lvlib:RCServoSetMaxPosition.vi

The maximum position `TargetPosition` can be set to.

- The units for `Position`,`Velocity`, and `Acceleration` are configured by scaling the internal timing (set with `MinPulseWidth` and `MaxPulseWidth`) to a user specified range with `MinPosition` and `MaxPosition`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Max Position The position value 1000_0 (ver: 200, 201) RC Servo Motor Controller: Def: 180 1000_0 (ver: 300, 312) RC Servo Motor Controller: Def: 180 1000_0 (ver: 313) RC Servo Motor Controller: Def: 180 1001_0 (ver: 200, 201) RC Servo Motor Controller: Def: 180 1001_0 (ver: 300, 302, 312) RC Servo Motor Controller: Def: 180 1001_0 (ver: 313) RC Servo Motor Controller: Def: 180 1001_0 (ver: 313, 400) RC Servo Motor Controller: Def: 180 1061_0 (ver: 100) RC Servo Motor Controller: Def: 180 1061_0 (ver: 200) RC Servo Motor Controller: Def: 180 1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Controller: Def: 180 1066_0 (ver: 100) RC Servo Motor Controller: Def: 180 1066_1 (ver: 100, 101) RC Servo Motor Controller: Def: 180 RCC1000_0 (ver: 106) RC Servo Motor Controller: Def: 180

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.