## Phidget Voltage Input.lvlib:VoltageInputSetVoltageRange.vi

The voltage range you choose should allow you to measure the full range of your input signal.

- A larger `VoltageRange` equates to less resolution.
- If a `Saturation` event occurs, increase the voltage range.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Voltage Range The voltage range value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
ADP1000_0 v104 | VCP1000_0 v100 | VCP1001_0 v100 | VCP1002_0 v106
VOLTAGE_RANGE_10mV | 1 | X | X | X | ✓
VOLTAGE_RANGE_40mV | 2 | X | X | X | ✓
VOLTAGE_RANGE_200mV | 3 | X | X | X | ✓
VOLTAGE_RANGE_312_5mV | 4 | X | ✓ | X | X
VOLTAGE_RANGE_400mV | 5 | ✓ | X | X | X
VOLTAGE_RANGE_1000mV | 6 | X | X | X | ✓
VOLTAGE_RANGE_2V | 7 | ✓ | X | X | X
VOLTAGE_RANGE_5V | 8 | X | X | ✓ | X
VOLTAGE_RANGE_15V | 9 | X | X | ✓ | X
VOLTAGE_RANGE_40V | 10 | X | ✓ | ✓ | X
VOLTAGE_RANGE_AUTO | 11 | X | X | ✓ | ✓
1011_0 (ver: 100, 101, 102, 103) Voltage Input: Unsupported 1013_0 (ver: 800, 811, 820) Voltage Input: Unsupported 1013_0 (ver: 821, 823) Voltage Input: Unsupported 1018_0 (ver: 824, 825, 826) Voltage Input: Unsupported 1018_1 (ver: 826) Voltage Input: Unsupported 1019_0 (ver: 826) Voltage Input: Unsupported 1070_0 (ver: 826) Voltage Input: Unsupported 1010_0 (ver: 903, 904) Voltage Input: Unsupported 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: Unsupported 1019_1 (ver: 903, 904) Voltage Input: Unsupported 1072_0 (ver: 903) Voltage Input: Unsupported 1073_0 (ver: 904) Voltage Input: Unsupported 1048_0 (ver: 100, 101, 102) Voltage Input: Unsupported 1051_0 (ver: 200, 201, 202) Voltage Input: Unsupported 1051_1 (ver: 300) Voltage Input: Unsupported 1051_2 (ver: 400, 401, 402) Voltage Input: Unsupported 1058_0 (ver: 100, 101) Voltage Input: Unsupported 1065_0 (ver: 100, 101) Voltage Input: Unsupported 1065_1 (ver: 100, 101) Voltage Input: Unsupported 1065_0 (ver: 100, 101) Supply Voltage Sensor: Unsupported 1065_1 (ver: 100, 101) Supply Voltage Sensor: Unsupported 1202_0 (ver: 100) Voltage Input: Unsupported 1203_0 (ver: 100) Voltage Input: Unsupported 1202_0 (ver: 120, 121) Voltage Input: Unsupported 1202_1 (ver: 123, 124) Voltage Input: Unsupported 1203_0 (ver: 120, 121) Voltage Input: Unsupported 1203_1 (ver: 123, 124) Voltage Input: Unsupported 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Unsupported 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Unsupported HUB0000_0 (ver: 117, 118, 119) Voltage Input: Unsupported SBC3003_0 (ver: 101, 102) Voltage Input: Unsupported HUB0000_0 (ver: 121) Voltage Input: Unsupported SBC3003_0 (ver: 108) Voltage Input: Unsupported ADP1000_0 (ver: 104) Voltage Input: Def: VOLTAGE_RANGE_400mV DAQ1000_0 (ver: 102, 103) Voltage Input: Unsupported DAQ1000_0 (ver: 110) Voltage Input: Unsupported DAQ1400_0 (ver: 112) Voltage Input: Unsupported SAF1000_0 (ver: 101, 102) Voltage Sensor: Unsupported TMP1100_0 (ver: 103, 105) Voltage Input: Unsupported TMP1101_0 (ver: 104, 106) Voltage Input: Unsupported VCP1000_0 (ver: 100) Voltage Input: Def: VOLTAGE_RANGE_40V VCP1001_0 (ver: 100) Voltage Input: Def: VOLTAGE_RANGE_AUTO VCP1002_0 (ver: 106) Voltage Input: Def: VOLTAGE_RANGE_AUTO

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.