## Phidget DC Motor.lvlib:DCMotorSetTargetVelocity.vi

The average voltage across the motor is based on the `TargetVelocity` value.

- At a constant load, increasing the target velocity will increase the speed of the motor.
- `TargetVelocity` is bounded by -1×`MaxVelocity` and `MaxVelocity`, where a sign change (±) is indicitave of a direction change.
- Setting `TargetVelocity` to `MinVelocity` will stop the motor. See `TargetBrakingStrength` for more information on stopping the motor.
- The units of `TargetVelocity` and `Acceleration` refer to 'duty cycle'. This is because the controller controls velocity by rapidly switching the power on/off (i.e. changing the duty cycle) in order to manipulate the voltage across the motor.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Target Velocity The velocity value Units: duty cycle (duty cycle) 1060_0 (ver: 100, 110) DC Motor Controller: Val: 0 1064_0 (ver: 100, 101, 102) DC Motor Controller: Val: 0 1064_1 (ver: 102) DC Motor Controller: Val: 0 1065_0 (ver: 100, 101) DC Motor Controller: Val: 0 1065_1 (ver: 100, 101) DC Motor Controller: Val: 0 DCC1000_0 (ver: 115) DC Motor Controller: DCC1000_0 (ver: 204, 205, 206) DC Motor Controller: DCC1001_0 (ver: 114, 116, 117) DC Motor Controller: DCC1002_0 (ver: 100) DC Motor Controller: DCC1003_0 (ver: 100) DC Motor Controller:

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.