## Phidget Accelerometer.lvlib:AccelerometerStart.vi

Opens and initializes a Phidget Accelerometer

| Change Trigger The change trigger value Units: g-force (g) 1008_0 (ver: 101) 2-Axis Accelerometer: Min: 0 Max: 4 Def: 0 1041_0 (ver: 200, 201, 202) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 1042_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 1043_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 1043_1 (ver: 302) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 1044_0 (ver: 400, 401, 402) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 1044_1 (ver: 500) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 1049_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 0 Max: 10 Def: 0 1053_0 (ver: 300, 301, 302) 2-Axis Accelerometer: Min: 0 Max: 10 Def: 0 1056_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 0 Max: 10 Def: 0 1056_0 (ver: 200) 3-Axis Accelerometer: Min: 0 Max: 10 Def: 0 1059_0 (ver: 400, 401) 3-Axis Accelerometer: Min: 0 Max: 6 Def: 0 MOT1100_0 (ver: 201, 202) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0 MOT1101_0 (ver: 112, 113) 3-Axis Accelerometer: Min: 0 Max: 16 Def: 0

| Data Interval The data interval value Units: milliseconds (ms) 1008_0 (ver: 101) 2-Axis Accelerometer: Min: 39 Max: 1000 Def: 273 1041_0 (ver: 200, 201, 202) 3-Axis Accelerometer: Min: 1 Max: 1000 Def: 256 1042_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: 4 Max: 1000 Def: 256 1043_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: 1 Max: 1000 Def: 256 1043_1 (ver: 302) 3-Axis Accelerometer: Min: 1 Max: 1000 Def: 256 1044_0 (ver: 400, 401, 402) 3-Axis Accelerometer: Min: 4 Max: 1000 Def: 256 1044_1 (ver: 500) 3-Axis Accelerometer: Min: 4 Max: 1000 Def: 256 1049_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 1 Max: 1000 Def: 256 1053_0 (ver: 300, 301, 302) 2-Axis Accelerometer: Min: 16 Max: 1000 Def: 256 1056_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 4 Max: 1000 Def: 256 1056_0 (ver: 200) 3-Axis Accelerometer: Min: 4 Max: 1000 Def: 256 1059_0 (ver: 400, 401) 3-Axis Accelerometer: Min: 16 Max: 1000 Def: 256 MOT1100_0 (ver: 201, 202) 3-Axis Accelerometer: Min: 10 Max: 60000 Def: 250 MOT1101_0 (ver: 112, 113) 3-Axis Accelerometer: Min: 20 Max: 60000 Def: 250

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number