## Phidget Magnetometer.lvlib:MagnetometerGetFieldStrength.vi

The most recent field strength value that the channel has reported.

- This value will always be between `MinMagneticField` and `MaxMagneticField`.

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device In Device # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| Field Strength The channel's measured MagneticField Units: gauss (G) 1042_0 (ver: 300, 301, 302) 3-Axis Magnetometer: Min: -5.6 Max: 5.6 1044_0 (ver: 400, 401, 402) 3-Axis Magnetometer: Min: -5.6 Max: 5.6 1044_1 (ver: 500) 3-Axis Magnetometer: Min: -50 Max: 50 1056_0 (ver: 100, 101, 102) 3-Axis Magnetometer: Min: -4 Max: 4 1056_0 (ver: 200) 3-Axis Magnetometer: Min: -4 Max: 4 MOT1101_0 (ver: 112, 113) 3-Axis Magnetometer: Min: -8 Max: 8

| Field Strength Field Strength