## Phidget LCD.lvlib:LCDDrawRect.vi

Draws a rectangle in the current frame buffer using the specified points

- Changes made to the frame buffer must be flushed to the LCD screen using `flush`.

Device Support:

1202_0 (ver: 100) Text LCD : Unsupported

1202_0 (ver: 120, 121) Text LCD : Unsupported

1202_1 (ver: 123, 124) Text LCD : Unsupported

1203_0 (ver: 100) Text LCD : Unsupported

1203_0 (ver: 120, 121) Text LCD : Unsupported

1203_1 (ver: 123, 124) Text LCD : Unsupported

1202_2 (ver: 200, 201, 202, 203, 204) Text LCD : Unsupported

1203_2 (ver: 200, 201, 202, 203, 204) Text LCD : Unsupported

1204_0 (ver: 100, 101) Text LCD : Unsupported

1215_0 (ver: 100, 101) Text LCD : Unsupported

1216_0 (ver: 100, 101) Text LCD : Unsupported

1217_0 (ver: 100, 101) Text LCD : Unsupported

1218_0 (ver: 100, 101) Text LCD : Unsupported

1219_0 (ver: 110, 111, 113) Text LCD : Unsupported

1220_0 (ver: 110, 111, 113) Text LCD : Unsupported

1221_0 (ver: 110, 111, 113) Text LCD : Unsupported

1222_0 (ver: 110, 111, 113) Text LCD : Unsupported

LCD1100_0 (ver: 106, 107, 108) Graphic LCD : Supported

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| x1 The X coordinate of the top-left corner of the rectangle

| y1 The Y coordinate of the top-left corner of the rectangle

| x2 The X coordinate of the bottom-right corner of the rectangle

| y2 The Y coordinate of the bottom-right corner of the rectangle

| filled If true, the rectangle will be solid. If false, just a single pixel outline.

| inverted If true, clears the region instead of drawing

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.