## Phidget Voltage Input.lvlib:VoltageInputVoltageEventExe.vi

The most recent voltage value the channel has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

- If a `VoltageChangeTrigger` has been set to a non-zero value, the `VoltageChange` event will not occur until the voltage has changed by at least the `VoltageChangeTrigger` value.
- If `SensorType` is supported and set to anything other then `SENSOR_TYPE_VOLTAGE`, this event will not fire.

Device Support:

1011_0 (ver: 100, 101, 102, 103) Voltage Input : Supported

1013_0 (ver: 800, 811, 820) Voltage Input : Supported

1013_0 (ver: 821, 823) Voltage Input : Supported

1018_0 (ver: 824, 825, 826) Voltage Input : Supported

1018_1 (ver: 826) Voltage Input : Supported

1019_0 (ver: 826) Voltage Input : Supported

1070_0 (ver: 826) Voltage Input : Supported

1010_0 (ver: 903, 904) Voltage Input : Supported

1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input : Supported

1019_1 (ver: 903, 904) Voltage Input : Supported

1072_0 (ver: 903) Voltage Input : Supported

1073_0 (ver: 904) Voltage Input : Supported

1018_3 (ver: 1000) Voltage Input : Supported

1048_0 (ver: 100, 101, 102) Voltage Input : Supported

1048_1 (ver: 200, 202, 204) Voltage Input : Supported

1048_2 (ver: 210, 212) Voltage Input : Supported

1051_0 (ver: 200, 201, 202) Voltage Input : Supported

1051_1 (ver: 300) Voltage Input : Supported

1051_2 (ver: 400, 401, 402) Voltage Input : Supported

1058_0 (ver: 100, 101) Voltage Input : Supported

1065_0 (ver: 100, 101) Voltage Input : Supported

1065_1 (ver: 100, 101) Voltage Input : Supported

1065_0 (ver: 100, 101) Supply Voltage Sensor : Supported

1065_1 (ver: 100, 101) Supply Voltage Sensor : Supported

1202_0 (ver: 100) Voltage Input : Supported

1203_0 (ver: 100) Voltage Input : Supported

1202_0 (ver: 120, 121) Voltage Input : Supported

1202_1 (ver: 123, 124) Voltage Input : Supported

1203_0 (ver: 120, 121) Voltage Input : Supported

1203_1 (ver: 123, 124) Voltage Input : Supported

1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input : Supported

1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input : Supported

HUB0000_0 (ver: 117, 118, 119) Voltage Input : Supported

HUB5000_0 (ver: 100) Voltage Input : Supported

SBC3003_0 (ver: 101, 102) Voltage Input : Supported

HUB0000_0 (ver: 121, 125, 126, 127) Voltage Input : Supported

HUB0000_0 (ver: 307) Voltage Input : Supported

HUB0001_0 (ver: 111) Voltage Input : Supported

HUB5000_0 (ver: 102, 104, 105, 106) Voltage Input : Supported

HUB5000_0 (ver: 107) Voltage Input : Supported

HUB5000_0 (ver: 203) Voltage Input : Supported

SBC3003_0 (ver: 108, 109, 110) Voltage Input : Supported

SBC3003_0 (ver: 203) Voltage Input : Supported

ADP1000_0 (ver: 104, 105) Voltage Input : Supported

DAQ1000_0 (ver: 102, 103) Voltage Input : Supported

DAQ1000_0 (ver: 110, 111, 112, 114) Voltage Input : Supported

DAQ1400_0 (ver: 112) Voltage Input : Supported

DAQ1400_0 (ver: 120, 121) Voltage Input : Supported

SAF1000_0 (ver: 101, 102) Voltage Sensor : Supported

SAF1000_0 (ver: 110) Voltage Sensor : Supported

STC1003_1 (ver: 201, 221) Voltage Input : Supported

TMP1100_0 (ver: 103, 105, 106, 108, 109) Voltage Input : Supported

TMP1101_0 (ver: 104, 106, 107, 109) Voltage Input : Supported

TMP1101_1 (ver: 201, 202, 203) Voltage Input : Supported

VCP1000_0 (ver: 100) Voltage Input : Supported

VCP1001_0 (ver: 100) Voltage Input : Supported

VCP1001_0 (ver: 110) Voltage Input : Supported

VCP1002_0 (ver: 106) Voltage Input : Supported

VCP1002_0 (ver: 110) Voltage Input : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| Voltage Measured voltage

| phid Device # Identification of the device that triggered the event.

| Event Registration Refnum Out Same as Event Registration Refnum In