## Phidget Temperature Sensor.lvlib:TemperatureSetRTDWireSetup.vi

The `RTDWireSetup` must correspond to the wire configuration you are using in your application.

- If you are unsure which `RTDWireSetup` to use, visit your device's User Guide for more information.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| RTD Wire Setup The RTD wire setup
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1045_0 v100 v101 | 1045_1 v101 | 1045_0 v100 v101 | 1045_1 v101 | 1048_0 v100 v101 v102 | 1048_0 v100 v101 v102 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1051_0 v100 | 1051_0 v100 | 1051_0 v200 v201 v202 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_1 v300 | 1051_2 v400 v401 v402 | 1051_2 v400 v401 v402 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | DCC1100_0 v113 v114 | DCC1100_0 v120 v121 v130 | HUM1000_0 v104 v105 | HUM1001_0 v102 | MOT0109_0 v112 v113 v115 v117 | MOT0110_0 v100 | MOT0110_0 v100 | SAF1000_0 v101 v102 | SAF1000_0 v110 | TMP1000_0 v105 v107 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_1 v201 v202 v203 | TMP1101_1 v201 v202 v203 | TMP1200_0 v104 v105 v106 v107 v108 v109 v110
RTD_WIRE_SETUP_2WIRE | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_WIRE_SETUP_3WIRE | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_WIRE_SETUP_4WIRE | 3 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
1045_0 (ver: 100, 101) Temperature Sensor (IR): Unsupported 1045_1 (ver: 101) Temperature Sensor (IR): Unsupported 1045_0 (ver: 100, 101) Temperature Sensor (IC): Unsupported 1045_1 (ver: 101) Temperature Sensor (IC): Unsupported 1048_0 (ver: 100, 101, 102) Thermocouple Input: Unsupported 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Unsupported 1048_1 (ver: 200, 202, 204) Thermocouple Input: Unsupported 1048_2 (ver: 210, 212) Thermocouple Input: Unsupported 1048_1 (ver: 200, 202, 204) Temperature Sensor (IC): Unsupported 1048_2 (ver: 210, 212) Temperature Sensor (IC): Unsupported 1051_0 (ver: 100) Thermocouple Input: Unsupported 1051_0 (ver: 100) Temperature Sensor (IC): Unsupported 1051_0 (ver: 200, 201, 202) Thermocouple Input: Unsupported 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Unsupported 1051_1 (ver: 300) Thermocouple Input: Unsupported 1051_1 (ver: 300) Temperature Sensor (IC): Unsupported 1051_2 (ver: 400, 401, 402) Thermocouple Input: Unsupported 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Unsupported DCC1000_0 (ver: 115) Temperature Sensor: Unsupported DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Unsupported DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Unsupported DCC1100_0 (ver: 113, 114) Temperature Sensor: Unsupported DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Unsupported HUM1000_0 (ver: 104, 105) Temperature Sensor: Unsupported HUM1001_0 (ver: 102) Temperature Sensor: Unsupported MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Unsupported MOT0110_0 (ver: 100) Temperature Sensor: Unsupported MOT0110_0 (ver: 100) Temperature Sensor: Unsupported SAF1000_0 (ver: 101, 102) Temperature Sensor: Unsupported SAF1000_0 (ver: 110) Temperature Sensor: Unsupported TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Unsupported TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Unsupported TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Unsupported TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Unsupported TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Unsupported TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Unsupported TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Unsupported TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Def: RTD_WIRE_SETUP_4WIRE

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.