## Phidget PH Sensor.lvlib:PHSensorStart.vi

Opens and initializes a Phidget PH Sensor

| Change Trigger The change trigger value Units: pH (pH) 1058_0 (ver: 100, 101) PH Input: Min: 0 Max: 14 Def: 0 ADP1000_0 (ver: 104, 105) PH Sensor Input: Min: 0 Max: 14 Def: 0

| Data Interval The data interval value Units: milliseconds (ms) 1058_0 (ver: 100, 101) PH Input: Min: 80 Max: 60000 Def: 256 ADP1000_0 (ver: 104, 105) PH Sensor Input: Min: 50 Max: 60000 Def: 250

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Correction Temperature The temperature of the solution to correct the pH measurement. Units: degrees celsius (°C) 1058_0 (ver: 100, 101) PH Input: Min: 0 Max: 100 Def: 25 ADP1000_0 (ver: 104, 105) PH Sensor Input: Min: 0 Max: 100 Def: 25

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number