## Phidget Digital Input.lvlib:DigitalInputSetInputMode.vi

The input polarity mode for your channel.

- See your device's User Guide for more information about what value to chooose for the `InputMode`

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Input Mode The input mode value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
| 1011_0 v100 v101 v102 v103 | 1012_0 v600 | 1012_0 v601 | 1012_0 v602 v603 v604 | 1012_1 v605 | 1012_2 v605 | 1012_3 v606 | 1013_0 v800 v811 v820 | 1013_0 v821 v823 | 1018_0 v824 v825 v826 | 1018_1 v826 | 1019_0 v826 | 1070_0 v826 | 1010_0 v903 v904 | 1018_2 v900 v901 v902 v903 v904 | 1019_1 v903 v904 | 1072_0 v903 | 1073_0 v904 | 1018_3 v1000 | 1047_0 v100 v101 v102 | 1047_1 v102 v103 | 1047_2 v200 | 1052_0 v100 | 1052_0 v101 v102 v103 | 1052_0 v110 v111 | 1060_0 v100 v110 | 1063_0 v100 | 1063_1 v100 v101 | 1065_0 v100 v101 | 1065_1 v100 v101 | 1202_0 v100 | 1203_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | 1219_0 v110 v111 v113 | 1220_0 v110 v111 v113 | 1221_0 v110 v111 v113 | 1222_0 v110 v111 v113 | HUB0000_0 v117 v118 v119 | HUB0000_0 v121 v125 v126 v127 | HUB0000_0 v307 | HUB0001_0 v111 | HUB5000_0 v100 | HUB5000_0 v102 v104 v105 v106 | HUB5000_0 v107 | HUB5000_0 v203 | SBC3003_0 v101 v102 | SBC3003_0 v108 v109 v110 | SBC3003_0 v203 | DAQ1200_0 v103 v104 | DAQ1300_0 v102 v103 | DAQ1301_0 v100 v102 | DAQ1400_0 v112 | DAQ1400_0 v120 v121 | HIN1101_0 v101 | HIN1100_0 v104 v105 v106
INPUT_MODE_NPN | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X
INPUT_MODE_PNP | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X

1011_0 (ver: 100, 101, 102, 103) Digital Input: Unsupported

1012_0 (ver: 600) Digital Input: Unsupported

1012_0 (ver: 601) Digital Input: Unsupported

1012_0 (ver: 602, 603, 604) Digital Input: Unsupported

1012_1 (ver: 605) Digital Input: Unsupported

1012_2 (ver: 605) Digital Input: Unsupported

1012_3 (ver: 606) Digital Input: Unsupported

1013_0 (ver: 800, 811, 820) Digital Input: Unsupported

1013_0 (ver: 821, 823) Digital Input: Unsupported

1018_0 (ver: 824, 825, 826) Digital Input: Unsupported

1018_1 (ver: 826) Digital Input: Unsupported

1019_0 (ver: 826) Digital Input: Unsupported

1070_0 (ver: 826) Digital Input: Unsupported

1010_0 (ver: 903, 904) Digital Input: Unsupported

1018_2 (ver: 900, 901, 902, 903, 904) Digital Input: Unsupported

1019_1 (ver: 903, 904) Digital Input: Unsupported

1072_0 (ver: 903) Digital Input: Unsupported

1073_0 (ver: 904) Digital Input: Unsupported

1018_3 (ver: 1000) Digital Input: Unsupported

1047_0 (ver: 100, 101, 102) Digital Input: Unsupported

1047_1 (ver: 102, 103) Digital Input: Unsupported

1047_2 (ver: 200) Digital Input: Unsupported

1052_0 (ver: 100) Digital Input: Unsupported

1052_0 (ver: 101, 102, 103) Digital Input: Unsupported

1052_0 (ver: 110, 111) Digital Input: Unsupported

1060_0 (ver: 100, 110) Digital Input: Unsupported

1063_0 (ver: 100) Digital Input: Unsupported

1063_1 (ver: 100, 101) Digital Input: Unsupported

1065_0 (ver: 100, 101) Digital Input: Unsupported

1065_1 (ver: 100, 101) Digital Input: Unsupported

1202_0 (ver: 100) Digital Input: Unsupported

1203_0 (ver: 100) Digital Input: Unsupported

1202_0 (ver: 120, 121) Digital Input: Unsupported

1202_1 (ver: 123, 124) Digital Input: Unsupported

1203_0 (ver: 120, 121) Digital Input: Unsupported

1203_1 (ver: 123, 124) Digital Input: Unsupported

1202_2 (ver: 200, 201, 202, 203, 204) Digital Input: Unsupported

1203_2 (ver: 200, 201, 202, 203, 204) Digital Input: Unsupported

1219_0 (ver: 110, 111, 113) Digital Input: Unsupported

1220_0 (ver: 110, 111, 113) Digital Input: Unsupported

1221_0 (ver: 110, 111, 113) Digital Input: Unsupported

1222_0 (ver: 110, 111, 113) Digital Input: Unsupported

HUB0000_0 (ver: 117, 118, 119) Digital Input: Unsupported

HUB0000_0 (ver: 121, 125, 126, 127) Digital Input: Unsupported

HUB0000_0 (ver: 307) Digital Input: Unsupported

HUB0001_0 (ver: 111) Digital Input: Unsupported

HUB5000_0 (ver: 100) Digital Input: Unsupported

HUB5000_0 (ver: 102, 104, 105, 106) Digital Input: Unsupported

HUB5000_0 (ver: 107) Digital Input: Unsupported

HUB5000_0 (ver: 203) Digital Input: Unsupported

SBC3003_0 (ver: 101, 102) Digital Input: Unsupported

SBC3003_0 (ver: 108, 109, 110) Digital Input: Unsupported

SBC3003_0 (ver: 203) Digital Input: Unsupported

DAQ1200_0 (ver: 103, 104) Digital Input: Unsupported

DAQ1300_0 (ver: 102, 103) Digital Input Isolated: Unsupported

DAQ1301_0 (ver: 100, 102) Digital Input Isolated: Unsupported

DAQ1400_0 (ver: 112) Digital Input: Def: INPUT_MODE_NPN

DAQ1400_0 (ver: 120, 121) Digital Input: Def: INPUT_MODE_NPN

HIN1101_0 (ver: 101) Digital Input: Def: INPUT_MODE_NPN

HIN1100_0 (ver: 104, 105, 106) Thumbstick Button: Def: INPUT_MODE_NPN

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.