## Phidget Accelerometer.lvlib:AccelerometerGetAxisCount.vi

The number of axes the channel can measure acceleration on.

- See your device's User Guide for more information about the number of axes and their orientation.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Axis Count The number of axes 1008_0 (ver: 101) 2-Axis Accelerometer: Val: 2 1041_0 (ver: 200, 201, 202) 3-Axis Accelerometer: Val: 3 1042_0 (ver: 300, 301, 302, 303) 3-Axis Accelerometer: Val: 3 1043_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Val: 3 1043_1 (ver: 302) 3-Axis Accelerometer: Val: 3 1044_0 (ver: 400, 401, 402, 403) 3-Axis Accelerometer: Val: 3 1044_1 (ver: 500, 502) 3-Axis Accelerometer: Val: 3 1044_1 (ver: 511) 3-Axis Accelerometer: Val: 3 1049_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Val: 3 1053_0 (ver: 300, 301, 302) 2-Axis Accelerometer: Val: 2 1056_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Val: 3 1056_0 (ver: 200) 3-Axis Accelerometer: Val: 3 1059_0 (ver: 400, 401) 3-Axis Accelerometer: Val: 3 MOT1100_0 (ver: 201, 202) 3-Axis Accelerometer: Val: 3 MOT1101_0 (ver: 112, 113) 3-Axis Accelerometer: Val: 3 MOT1102_0 (ver: 210, 212) 3-Axis Accelerometer: Val: 3 MOT1102_1 (ver: 300) 3-Axis Accelerometer: Val: 3 MOT0109_0 (ver: 112, 113, 115, 117) 3-Axis Accelerometer: Val: 3 MOT0110_0 (ver: 100) 3-Axis Accelerometer: Val: 3 MOT0110_0 (ver: 100) 3-Axis Accelerometer: Val: 3