## Phidget Current Input.lvlib:CurrentInputStart.vi

Opens and initializes a Phidget Current Input

| Change Trigger The change trigger value Units: amperes (A) 1061_0 (ver: 100) RC Servo Motor Current Sensor: Min: 0 Max: 1 Def: 0 1061_0 (ver: 200) RC Servo Motor Current Sensor: Min: 0 Max: 1 Def: 0 1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Current Sensor: Min: 0 Max: 1 Def: 0 1063_0 (ver: 100) Bipolar Stepper Current Sensor: Min: 0 Max: 1 Def: 0 1063_1 (ver: 100, 101) Bipolar Stepper Current Sensor: Min: 0 Max: 1 Def: 0 1064_0 (ver: 100, 101, 102) DC Motor Current Sensor: Min: 0 Max: 1 Def: 0 1064_1 (ver: 102) DC Motor Current Sensor: Min: 0 Max: 1 Def: 0 1065_0 (ver: 100, 101) DC Motor Current Sensor: Min: 0 Max: 1 Def: 0 1065_1 (ver: 100, 101) DC Motor Current Sensor: Min: 0 Max: 1 Def: 0 1066_0 (ver: 100) RC Servo Motor Current Sensor: Min: 0 Max: 1 Def: 0 1066_1 (ver: 100, 101) RC Servo Motor Current Sensor: Min: 0 Max: 1 Def: 0 DAQ1400_0 (ver: 112) Current Input: Min: 0 Max: 0.016 Def: 0 DAQ1400_0 (ver: 120, 121) Current Input: Min: 0 Max: 0.016 Def: 0 VCP1100_0 (ver: 101) Current Input: Min: 0 Max: 60 Def: 0 DCC1000_0 (ver: 115) Current Sensor: Min: 0 Max: 25Val: 0 DCC1000_0 (ver: 204, 205, 206) Current Sensor: Min: 0 Max: 25Val: 0 DCC1000_0 (ver: 210, 211, 220) Current Sensor: Min: 0 Max: 25Val: 0

| Data Interval The data interval value Units: milliseconds (ms) 1061_0 (ver: 100) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1061_0 (ver: 200) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1063_0 (ver: 100) Bipolar Stepper Current Sensor: Min: 8 Max: 60000 Def: 256 1063_1 (ver: 100, 101) Bipolar Stepper Current Sensor: Min: 8 Max: 60000 Def: 256 1064_0 (ver: 100, 101, 102) DC Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1064_1 (ver: 102) DC Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1065_0 (ver: 100, 101) DC Motor Current Sensor: Min: 8 Max: 60000 Def: 256 1065_1 (ver: 100, 101) DC Motor Current Sensor: Min: 8 Max: 60000 Def: 256 1066_0 (ver: 100) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1066_1 (ver: 100, 101) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 DAQ1400_0 (ver: 112) Current Input: Min: 20 Max: 60000 Def: 250 DAQ1400_0 (ver: 120, 121) Current Input: Min: 20 Max: 60000 Def: 250 VCP1100_0 (ver: 101) Current Input: Min: 20 Max: 60000 Def: 250 DCC1000_0 (ver: 115) Current Sensor: Min: 100 Max: 60000Val: 250 DCC1000_0 (ver: 204, 205, 206) Current Sensor: Min: 100 Max: 60000Val: 250 DCC1000_0 (ver: 210, 211, 220) Current Sensor: Min: 100 Max: 60000Val: 250

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number