## Phidget Encoder.lvlib:EncoderEventExe.vi

The most recent values the channel has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

- If a `PositionChangeTrigger` has been set to a non-zero value, the `PositionChange` event will not occur until the position has changed by at least the `PositionChangeTrigger` value.

Device Support:

1047_0 (ver: 100, 101, 102) Encoder Input : Supported

1047_1 (ver: 102, 103) Encoder Input : Supported

1047_2 (ver: 200) Encoder Input : Supported

1052_0 (ver: 100) Encoder Input : Supported

1052_0 (ver: 101, 102, 103) Encoder Input : Supported

1052_0 (ver: 110, 111) Encoder Input : Supported

1057_0 (ver: 300, 301) Encoder Input : Supported

1057_1 (ver: 302) Encoder Input : Supported

1057_2 (ver: 302) Encoder Input : Supported

1057_3 (ver: 400) Encoder Input : Supported

1065_0 (ver: 100, 101) Encoder Input : Supported

1065_1 (ver: 100, 101) Encoder Input : Supported

DCC1000_0 (ver: 115) Encoder Input : Supported

DCC1000_0 (ver: 204, 205, 206) Encoder Input : Supported

DCC1000_0 (ver: 210, 211, 220) Encoder Input : Supported

DCC1001_0 (ver: 114, 116, 117) Encoder Input : Supported

DCC1001_0 (ver: 120, 130) Encoder Input : Supported

DCC1002_0 (ver: 100, 101, 102) Encoder Input : Supported

DCC1002_0 (ver: 111, 120) Encoder Input : Supported

ENC1000_0 (ver: 101) Encoder Input : Supported

HIN1101_0 (ver: 101) Encoder Input : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| phid Device # Identification of the device that triggered the event.

| Enc Index Trigged True if the index was passed since the last change event

| Time Change The time elapsed since the last change event in milliseconds

| Pos Change The amount the position changed since the last change event

| Event Registration Refnum Out Same as Event Registration Refnum In