## Phidget DC Motor.lvlib:DCMotorSetAcceleration.vi

The rate at which the controller can change the motor's `Velocity`.

- The acceleration is bounded by `MinAcceleration` and `MaxAcceleration`

  | Device In Device # Identification

  | error in (no error) error in can accept error information wired from VIs previously called.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | Acceleration The acceleration value Units: duty cycle per second (duty cycle/s) 1060_0 (ver: 100, 110) DC Motor Controller: Min: 0.0122 Max: 12.45 Def: 1 1064_0 (ver: 100, 101, 102) DC Motor Controller: Min: 0.019 Max: 19.4 Def: 1 1064_1 (ver: 102) DC Motor Controller: Min: 0.019 Max: 19.4 Def: 1 1065_0 (ver: 100, 101) DC Motor Controller: Min: 0.2778 Max: 62.5 Def: 1 1065_1 (ver: 100, 101) DC Motor Controller: Min: 0.2778 Max: 62.5 Def: 1 DCC1000_0 (ver: 115) DC Motor Controller: Min: 0.1 Max: 100Val: 1 DCC1000_0 (ver: 204, 205, 206) DC Motor Controller: Min: 0.1 Max: 100Val: 1 DCC1000_0 (ver: 210, 211, 220) DC Motor Controller: Min: 0.1 Max: 100Val: 1 DCC1001_0 (ver: 114, 116, 117) DC Motor Controller: Min: 0.1 Max: 100 Def: 1 DCC1001_0 (ver: 120, 130) DC Motor Controller: Min: 0.1 Max: 100 Def: 1 DCC1002_0 (ver: 100, 101, 102) DC Motor Controller: Min: 0.1 Max: 100 Def: 1 DCC1002_0 (ver: 111, 120) DC Motor Controller: Min: 0.1 Max: 100 Def: 1 DCC1003_0 (ver: 100, 101, 102) DC Motor Controller: Min: 0.1 Max: 100 Def: 1 DCC1003_0 (ver: 110, 120) DC Motor Controller: Min: 0.1 Max: 100 Def: 1

  | Device Out Same as Device In

  | error out error out passes error or warning information out of a VI to be used by other VIs.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.