## Phidget Motor Position Controller.lvlib:MotorPositionControllerSetFanMode.vi

The `FanMode` dictates the operating condition of the fan.

- Choose between on, off, or automatic (based on temperature).
- If the `FanMode` is set to automatic, the fan will turn on when the temperature reaches 70°C and it will remain on until the temperature falls below 55°C.
- If the `FanMode` is off, the controller will still turn on the fan if the temperature reaches 85°C and it will remain on until it falls below 70°C.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Fan Mode The fan mode
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | DCC1001_0 v114 v116 v117 | DCC1001_0 v120 v130 | DCC1002_0 v100 v101 v102 | DCC1002_0 v111 v120 | DCC1100_0 v113 v114 | DCC1100_0 v120 v121 v130
FAN_MODE_OFF | 1 | ✓ | ✓ | X | X | X | X | X | X
FAN_MODE_ON | 2 | ✓ | ✓ | X | X | X | X | X | X
FAN_MODE_AUTO | 3 | ✓ | ✓ | X | X | X | X | X | X
DCC1000_0 (ver: 204, 205, 206) Position Controller: Val: FAN_MODE_AUTO DCC1000_0 (ver: 210, 211, 220) Position Controller: Val: FAN_MODE_AUTO DCC1001_0 (ver: 114, 116, 117) Position Controller: Val: FAN_MODE_AUTO DCC1001_0 (ver: 120, 130) Position Controller: Val: FAN_MODE_AUTO DCC1002_0 (ver: 100, 101, 102) Position Controller: Val: FAN_MODE_AUTO DCC1002_0 (ver: 111, 120) Position Controller: Val: FAN_MODE_AUTO DCC1100_0 (ver: 113, 114) Position Controller: Val: FAN_MODE_AUTO DCC1100_0 (ver: 120, 121, 130) Position Controller: Val: FAN_MODE_AUTO

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.