## Phidget Temperature Sensor.lvlib:TemperatureSensorStart.vi

Opens and initializes a Phidget Temperature Sensor

| Change Trigger The change trigger value Units: degrees celsius (°C) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Min: 0 Max: 1000 Def: 0 1045_1 (ver: 101) Temperature Sensor (IR): Min: 0 Max: 1000 Def: 0 1045_0 (ver: 100, 101) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1045_1 (ver: 101) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1048_0 (ver: 100, 101, 102) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1048_1 (ver: 200, 202, 204) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1048_2 (ver: 210, 212) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1048_1 (ver: 200, 202, 204) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1048_2 (ver: 210, 212) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_0 (ver: 100) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_0 (ver: 100) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_0 (ver: 200, 201, 202) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_1 (ver: 300) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_1 (ver: 300) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 1051_2 (ver: 400, 401, 402) Thermocouple Input: Min: 0 Max: 1000 Def: 0 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Min: 0 Max: 100 Def: 0 DCC1000_0 (ver: 115) Temperature Sensor: Min: 0 Max: 165Val: 0 DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Min: 0 Max: 165Val: 0 DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Min: 0 Max: 165Val: 0 DCC1100_0 (ver: 113, 114) Temperature Sensor: Min: 0 Max: 165 Def: 0 DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Min: 0 Max: 165 Def: 0 HUM1000_0 (ver: 104, 105) Temperature Sensor: Min: 0 Max: 125 Def: 0 HUM1001_0 (ver: 102) Temperature Sensor: Min: 0 Max: 125 Def: 0 MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Min: 0 Max: 125 Def: 0 MOT0110_0 (ver: 100) Temperature Sensor: Min: 0 Max: 125 Def: 0 MOT0110_0 (ver: 100) Temperature Sensor: Min: 0 Max: 125 Def: 0 SAF1000_0 (ver: 101, 102) Temperature Sensor: Min: 0 Max: 165 Def: 0 SAF1000_0 (ver: 110) Temperature Sensor: Min: 0 Max: 165 Def: 0 TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Min: 0 Max: 125Val: 0 TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Min: 0 Max: 1640 Def: 0 TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Min: 0 Max: 125 Def: 0 TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Min: 0 Max: 1640 Def: 0 TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Min: 0 Max: 125 Def: 0 TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Min: 0 Max: 1640 Def: 0 TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Min: 0 Max: 125 Def: 0 TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Min: 0 Max: 1050 Def: 0

| Data Interval The data interval value Units: milliseconds (ms) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Min: 32 Max: 60000 Def: 256 1045_1 (ver: 101) Temperature Sensor (IR): Min: 32 Max: 60000 Def: 256 1045_0 (ver: 100, 101) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1045_1 (ver: 101) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_0 (ver: 100, 101, 102) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_1 (ver: 200, 202, 204) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_2 (ver: 210, 212) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_1 (ver: 200, 202, 204) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_2 (ver: 210, 212) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_0 (ver: 100) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 100) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 DCC1000_0 (ver: 115) Temperature Sensor: Min: 500 Max: 60000Val: 500 DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Min: 500 Max: 60000Val: 500 DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Min: 500 Max: 60000Val: 500 DCC1100_0 (ver: 113, 114) Temperature Sensor: Min: 100 Max: 60000 Def: 250 DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Min: 100 Max: 60000 Def: 250 HUM1000_0 (ver: 104, 105) Temperature Sensor: Min: 500 Max: 60000 Def: 500 HUM1001_0 (ver: 102) Temperature Sensor: Min: 50 Max: 60000 Def: 250 MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Min: 100 Max: 60000 Def: 250 MOT0110_0 (ver: 100) Temperature Sensor: Min: 10 Max: 60000 Def: 250 MOT0110_0 (ver: 100) Temperature Sensor: Min: 10 Max: 60000 Def: 250 SAF1000_0 (ver: 101, 102) Temperature Sensor: Min: 100 Max: 60000 Def: 250 SAF1000_0 (ver: 110) Temperature Sensor: Min: 100 Max: 60000 Def: 250 TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Min: 500 Max: 60000Val: 500 TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Min: 250 Max: 60000 Def: 250

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| ThermocoupleType The thermocouple type
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1045_0 v100 v101 | 1045_1 v101 | 1045_0 v100 v101 | 1045_1 v101 | 1048_0 v100 v101 v102 | 1048_0 v100 v101 v102 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1051_0 v100 | 1051_0 v100 | 1051_0 v200 v201 v202 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_1 v300 | 1051_2 v400 v401 v402 | 1051_2 v400 v401 v402 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | DCC1100_0 v113 v114 | DCC1100_0 v120 v121 v130 | HUM1000_0 v104 v105 | HUM1001_0 v102 | MOT0109_0 v112 v113 v115 v117 | MOT0110_0 v100 | MOT0110_0 v100 | SAF1000_0 v101 v102 | SAF1000_0 v110 | TMP1000_0 v105 v107 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_1 v201 v202 v203 | TMP1101_1 v201 v202 v203 | TMP1200_0 v104 v105 v106 v107 v108 v109 v110
THERMOCOUPLE_TYPE_J | 1 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X
THERMOCOUPLE_TYPE_K | 2 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | ✓ | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X
THERMOCOUPLE_TYPE_E | 3 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X
THERMOCOUPLE_TYPE_T | 4 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X
1045_0 (ver: 100, 101) Temperature Sensor (IR): Unsupported 1045_1 (ver: 101) Temperature Sensor (IR): Unsupported 1045_0 (ver: 100, 101) Temperature Sensor (IC): Unsupported 1045_1 (ver: 101) Temperature Sensor (IC): Unsupported 1048_0 (ver: 100, 101, 102) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1048_1 (ver: 200, 202, 204) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_2 (ver: 210, 212) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_1 (ver: 200, 202, 204) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1048_2 (ver: 210, 212) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1051_0 (ver: 100) Thermocouple Input: Val: THERMOCOUPLE_TYPE_K 1051_0 (ver: 100) Temperature Sensor (IC): Val: THERMOCOUPLE_TYPE_K 1051_0 (ver: 200, 201, 202) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1051_1 (ver: 300) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_1 (ver: 300) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1051_2 (ver: 400, 401, 402) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K DCC1000_0 (ver: 115) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1100_0 (ver: 113, 114) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K HUM1000_0 (ver: 104, 105) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K HUM1001_0 (ver: 102) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K MOT0110_0 (ver: 100) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K MOT0110_0 (ver: 100) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K SAF1000_0 (ver: 101, 102) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K SAF1000_0 (ver: 110) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Def: THERMOCOUPLE_TYPE_K

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| RTD Type The RTD type
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1045_0 v100 v101 | 1045_1 v101 | 1045_0 v100 v101 | 1045_1 v101 | 1048_0 v100 v101 v102 | 1048_0 v100 v101 v102 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1051_0 v100 | 1051_0 v100 | 1051_0 v200 v201 v202 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_1 v300 | 1051_2 v400 v401 v402 | 1051_2 v400 v401 v402 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | DCC1100_0 v113 v114 | DCC1100_0 v120 v121 v130 | HUM1000_0 v104 v105 | HUM1001_0 v102 | MOT0109_0 v112 v113 v115 v117 | MOT0110_0 v100 | MOT0110_0 v100 | SAF1000_0 v101 v102 | SAF1000_0 v110 | TMP1000_0 v105 v107 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_1 v201 v202 v203 | TMP1101_1 v201 v202 v203 | TMP1200_0 v104 v105 v106 v107 v108 v109 v110
RTD_TYPE_PT100_3850 | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_TYPE_PT1000_3850 | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_TYPE_PT100_3920 | 3 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_TYPE_PT1000_3920 | 4 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
1045_0 (ver: 100, 101) Temperature Sensor (IR): Unsupported 1045_1 (ver: 101) Temperature Sensor (IR): Unsupported 1045_0 (ver: 100, 101) Temperature Sensor (IC): Unsupported 1045_1 (ver: 101) Temperature Sensor (IC): Unsupported 1048_0 (ver: 100, 101, 102) Thermocouple Input: Unsupported 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Unsupported 1048_1 (ver: 200, 202, 204) Thermocouple Input: Unsupported 1048_2 (ver: 210, 212) Thermocouple Input: Unsupported 1048_1 (ver: 200, 202, 204) Temperature Sensor (IC): Unsupported 1048_2 (ver: 210, 212) Temperature Sensor (IC): Unsupported 1051_0 (ver: 100) Thermocouple Input: Unsupported 1051_0 (ver: 100) Temperature Sensor (IC): Unsupported 1051_0 (ver: 200, 201, 202) Thermocouple Input: Unsupported 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Unsupported 1051_1 (ver: 300) Thermocouple Input: Unsupported 1051_1 (ver: 300) Temperature Sensor (IC): Unsupported 1051_2 (ver: 400, 401, 402) Thermocouple Input: Unsupported 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Unsupported DCC1000_0 (ver: 115) Temperature Sensor: Unsupported DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Unsupported DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Unsupported DCC1100_0 (ver: 113, 114) Temperature Sensor: Unsupported DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Unsupported HUM1000_0 (ver: 104, 105) Temperature Sensor: Unsupported HUM1001_0 (ver: 102) Temperature Sensor: Unsupported MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Unsupported MOT0110_0 (ver: 100) Temperature Sensor: Unsupported MOT0110_0 (ver: 100) Temperature Sensor: Unsupported SAF1000_0 (ver: 101, 102) Temperature Sensor: Unsupported SAF1000_0 (ver: 110) Temperature Sensor: Unsupported TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Unsupported TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Unsupported TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Unsupported TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Unsupported TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Unsupported TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Unsupported TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Unsupported TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Def: RTD_TYPE_PT1000_3850

| RTD Wire Setup The RTD wire setup
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1045_0 v100 v101 | 1045_1 v101 | 1045_0 v100 v101 | 1045_1 v101 | 1048_0 v100 v101 v102 | 1048_0 v100 v101 v102 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1048_1 v200 v202 v204 | 1048_2 v210 v212 | 1051_0 v100 | 1051_0 v100 | 1051_0 v200 v201 v202 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_1 v300 | 1051_2 v400 v401 v402 | 1051_2 v400 v401 v402 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | DCC1100_0 v113 v114 | DCC1100_0 v120 v121 v130 | HUM1000_0 v104 v105 | HUM1001_0 v102 | MOT0109_0 v112 v113 v115 v117 | MOT0110_0 v100 | MOT0110_0 v100 | SAF1000_0 v101 v102 | SAF1000_0 v110 | TMP1000_0 v105 v107 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_1 v201 v202 v203 | TMP1101_1 v201 v202 v203 | TMP1200_0 v104 v105 v106 v107 v108 v109 v110
RTD_WIRE_SETUP_2WIRE | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_WIRE_SETUP_3WIRE | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
RTD_WIRE_SETUP_4WIRE | 3 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
1045_0 (ver: 100, 101) Temperature Sensor (IR): Unsupported 1045_1 (ver: 101) Temperature Sensor (IR): Unsupported 1045_0 (ver: 100, 101) Temperature Sensor (IC): Unsupported 1045_1 (ver: 101) Temperature Sensor (IC): Unsupported 1048_0 (ver: 100, 101, 102) Thermocouple Input: Unsupported 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Unsupported 1048_1 (ver: 200, 202, 204) Thermocouple Input: Unsupported 1048_2 (ver: 210, 212) Thermocouple Input: Unsupported 1048_1 (ver: 200, 202, 204) Temperature Sensor (IC): Unsupported 1048_2 (ver: 210, 212) Temperature Sensor (IC): Unsupported 1051_0 (ver: 100) Thermocouple Input: Unsupported 1051_0 (ver: 100) Temperature Sensor (IC): Unsupported 1051_0 (ver: 200, 201, 202) Thermocouple Input: Unsupported 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Unsupported 1051_1 (ver: 300) Thermocouple Input: Unsupported 1051_1 (ver: 300) Temperature Sensor (IC): Unsupported 1051_2 (ver: 400, 401, 402) Thermocouple Input: Unsupported 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Unsupported DCC1000_0 (ver: 115) Temperature Sensor: Unsupported DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Unsupported DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Unsupported DCC1100_0 (ver: 113, 114) Temperature Sensor: Unsupported DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Unsupported HUM1000_0 (ver: 104, 105) Temperature Sensor: Unsupported HUM1001_0 (ver: 102) Temperature Sensor: Unsupported MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Unsupported MOT0110_0 (ver: 100) Temperature Sensor: Unsupported MOT0110_0 (ver: 100) Temperature Sensor: Unsupported SAF1000_0 (ver: 101, 102) Temperature Sensor: Unsupported SAF1000_0 (ver: 110) Temperature Sensor: Unsupported TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Unsupported TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Unsupported TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Unsupported TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Unsupported TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Unsupported TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Unsupported TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Unsupported TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Def: RTD_WIRE_SETUP_4WIRE

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number