## Phidget Frequency Counter.lvlib:FrequencyCounterGetFrequency.vi

The most recent frequency value that the channel has reported.

- This value will always be between 0 Hz and `MaxFrequency`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Frequency The frequency value Units: hertz (Hz) 1054_0 (ver: 100, 101) Frequency Input: Max: 1000000Val: 0 DAQ1400_0 (ver: 112) Frequency Input: Max: 1000000Val: 0 DAQ1400_0 (ver: 120, 121) Frequency Input: Max: 1000000Val: 0