## Phidget Spatial.lvlib:SpatialStart.vi

Opens and initializes a Phidget Spatial

| Data Interval The data interval value Units: milliseconds (ms) 1042_0 (ver: 300, 301, 302, 303) Spatial: Min: 4 Max: 1000 Def: 256 1044_0 (ver: 400, 401, 402, 403) Spatial: Min: 4 Max: 1000 Def: 256 1044_1 (ver: 500, 502) Spatial: Min: 4 Max: 1000 Def: 256 1044_1 (ver: 511) Spatial: Min: 4 Max: 1000 Def: 256 1056_0 (ver: 100, 101, 102) Spatial: Min: 4 Max: 1000 Def: 256 1056_0 (ver: 200) Spatial: Min: 4 Max: 1000 Def: 256 MOT1101_0 (ver: 112, 113) Spatial: Min: 20 Max: 60000 Def: 250 MOT1102_0 (ver: 210, 212) Spatial: Min: 20 Max: 60000 Def: 250 MOT1102_1 (ver: 300) Spatial: Min: 20 Max: 60000 Def: 250 MOT0109_0 (ver: 112, 113, 115, 117) Spatial: Min: 4 Max: 1000 Def: 256 MOT0110_0 (ver: 100) Spatial: Min: 1 Max: 1000 Def: 250 MOT0110_0 (ver: 100) Spatial: Min: 2 Max: 1000 Def: 250

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number