## Phidget Power Guard.lvlib:PowerGuardStart.vi

Opens and initializes a Phidget Power Guard

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Over Voltage The voltage value Units: volts (V) SAF1000_0 (ver: 101, 102) Power Supply Protector: Min: 8 Max: 33 SAF1000_0 (ver: 110) Power Supply Protector: Min: 8 Max: 33

| Fan Mode The fan mode value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
SAF1000_0 v101 v102 | SAF1000_0 v110
FAN_MODE_OFF | 1 | ✓ | ✓
FAN_MODE_ON | 2 | ✓ | ✓
FAN_MODE_AUTO | 3 | ✓ | ✓
SAF1000_0 (ver: 101, 102) Power Supply Protector: Def: FAN_MODE_AUTO SAF1000_0 (ver: 110) Power Supply Protector: Def: FAN_MODE_AUTO

| Power Enabled The power enabled value. SAF1000_0 (ver: 101, 102) Power Supply Protector: Def: 0 SAF1000_0 (ver: 110) Power Supply Protector: Def: 0

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number