## Phidget Motor Position Controller.lvlib:MotorPositionControllerPositionChangeEventExe.vi

The most recent position value will be reported in this event, which occurs when the `DataInterval` has elapsed.

- Regardless of the `DataInterval`, this event will occur only when the position value has changed from the previous value reported.
- Units for `Position` can be set by the user through the `RescaleFactor`. The `RescaleFactor` allows you to use more intuitive units such as rotations, or degrees.

  Device Support:

  DCC1000_0 (ver: 204, 205, 206) Position Controller : Supported

  DCC1000_0 (ver: 210, 211, 220) Position Controller : Supported

  DCC1001_0 (ver: 114, 116, 117) Position Controller : Supported

  DCC1001_0 (ver: 120, 130) Position Controller : Supported

  DCC1002_0 (ver: 100, 101, 102) Position Controller : Supported

  DCC1002_0 (ver: 111, 120) Position Controller : Supported

  DCC1100_0 (ver: 113, 114) Position Controller : Supported

  DCC1100_0 (ver: 120, 121, 130) Position Controller : Supported

  | error in (no error) error in can accept error information wired from VIs previously called.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | Devices In A list of devices registered for the same type of event

  | Device In Device # Identification

  | Event Registration Refnum In Event # Identification

  | error out error out passes error or warning information out of a VI to be used by other VIs.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | Event? Returns TRUE if the event has executed, or FALSE otherwise.

  | Devices Out Same as Devices In

  | Device Out Same as Device In

  | Index The index of the device that triggered the event within the Devices In array.

  | phid Device # Identification of the device that triggered the event.

  | Position The position value

  | Event Registration Refnum Event # Identification