## Phidget RFID.lvlib:RFID_TagLostEventExe.vi

Occurs when an RFID tag that was being read is no longer seen by the reader. Typically this indicates the tag has been removed from the read range, though it could also happen due to interference from multiple tags entering the read range at the same time.

Device Support:

1023_0 (ver: 103) RFID Reader : Supported

1023_0 (ver: 104) RFID Reader : Supported

1023_0 (ver: 200) RFID Reader : Supported

1023_0 (ver: 201, 202, 203, 204) RFID Reader : Supported

1023_1 (ver: 205, 206) RFID Reader : Supported

1024_0 (ver: 100, 101, 103) RFID Reader/Writer : Supported

1024_1 (ver: 301) RFID Reader/Writer : Supported

1024_1 (ver: 301) RFID Reader/Writer : Supported

1024_1 (ver: 310) RFID Reader/Writer : Supported

1024_1 (ver: 310) RFID Reader/Writer : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| phid Device # Identification of the device that triggered the event.

| Protocol Communication protocol of the lost tag
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1023_0 v103 | 1023_0 v104 | 1023_0 v200 | 1023_0 v201 v202 v203 v204 | 1023_1 v205 v206 | 1024_0 v100 v101 v103 | 1024_1 v301 | 1024_1 v301 | 1024_1 v310 | 1024_1 v310
PROTOCOL_EM4100 | 1 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
PROTOCOL_ISO11785_FDX_B | 2 | X | X | X | X | X | ✓ | ✓ | ✓ | ✓ | ✓
PROTOCOL_PHIDGETS | 3 | X | X | X | X | X | ✓ | ✓ | ✓ | ✓ | ✓
PROTOCOL_HID_GENERIC | 4 | X | X | X | X | X | X | X | X | ✓ | ✓
PROTOCOL_HID_H10301 | 5 | X | X | X | X | X | X | X | X | ✓ | ✓

| Tag String Data from the lost tag

| Event Registration Refnum Out Same as Event Registration Refnum In