## Phidget Stepper.lvlib:StepperSetDataInterval.vi

The `DataInterval` is the time that must elapse before the channel will fire another `PositionChange` / `VelocityChange` event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1062_0 (ver: 101) Unipolar Stepper Controller: Min: 16 Max: 60000 Def: 256 1062_1 (ver: 101, 102) Unipolar Stepper Controller: Min: 16 Max: 60000 Def: 256 1063_0 (ver: 100) Bipolar Stepper Controller: Min: 8 Max: 60000 Def: 256 1063_1 (ver: 100, 101) Bipolar Stepper Controller: Min: 8 Max: 60000 Def: 256 1067_0 (ver: 200, 201, 202, 203, 204, 205, 206) Bipolar Stepper Controller: Min: 8 Max: 60000 Def: 256 STC1000_0 (ver: 100, 101) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1000_0 (ver: 110, 111, 112, 113, 114, 121) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1001_0 (ver: 100, 101) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1001_0 (ver: 110, 111, 112, 113, 114, 115, 121) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1002_0 (ver: 101, 102) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1002_0 (ver: 110, 111, 112, 113, 114, 121) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1003_0 (ver: 100, 101) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1003_0 (ver: 110, 111, 112, 113, 114, 121) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250 STC1003_1 (ver: 201, 221) Bipolar Stepper Controller: Min: 100 Max: 60000 Def: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.