## Phidget Voltage Ratio Input.lvlib:VoltageRatioInputSetBridgeGain.vi

Choose a `BridgeGain` that best suits your application.

- For more information about the range and accuracy of each `BridgeGain` to decide which best suits your application, see your device's User Guide.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Bridge Gain The bridge gain value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
| 1011_0 v100 v101 v102 v103 | 1013_0 v800 v811 v820 | 1013_0 v821 v823 | 1018_0 v824 v825 v826 | 1018_1 v826 | 1019_0 v826 | 1070_0 v826 | 1010_0 v903 v904 | 1018_2 v900 v901 v902 v903 v904 | 1019_1 v903 v904 | 1072_0 v903 | 1073_0 v904 | 1018_3 v1000 v1001 | 1046_0 v100 v101 | 1046_0 v102 | 1046_1 v200 v201 | 1065_0 v100 v101 | 1065_1 v100 v101 | 1202_0 v100 | 1203_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | HUB0000_0 v117 v118 v119 | HUB0000_0 v121 v125 v126 v127 | HUB0000_0 v307 | HUB0001_0 v111 v113 v114 | HUB0001_0 v115 v116 | HUB5000_0 v100 | HUB5000_0 v102 v104 v105 v106 | HUB5000_0 v107 | HUB5000_0 v203 v204 v205 | SBC3003_0 v101 v102 | SBC3003_0 v108 v109 v110 | SBC3003_0 v203 v204 | HUB0000_1 v400 v401 | HUB0002_0 v100 v101 | HUB0007_0 v101 v102 | DAQ1000_0 v102 v103 | DAQ1000_0 v110 v111 v112 v114 | DAQ1500_0 v104 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | HIN1100_0 v104 v105 v106 | HUM1100_0 v100 | HUM1100_1 v100
BRIDGE_GAIN_1 | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X
BRIDGE_GAIN_2 | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X
BRIDGE_GAIN_4 | 3 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X
BRIDGE_GAIN_8 | 4 | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X
BRIDGE_GAIN_16 | 5 | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X
BRIDGE_GAIN_32 | 6 | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X
BRIDGE_GAIN_64 | 7 | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X
BRIDGE_GAIN_128 | 8 | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X

1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Unsupported

1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Unsupported

1013_0 (ver: 821, 823) Voltage Ratio Input: Unsupported

1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Unsupported

1018_1 (ver: 826) Voltage Ratio Input: Unsupported

1019_0 (ver: 826) Voltage Ratio Input: Unsupported

1070_0 (ver: 826) Voltage Ratio Input: Unsupported

1010_0 (ver: 903, 904) Voltage Ratio Input: Unsupported

1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Unsupported

1019_1 (ver: 903, 904) Voltage Ratio Input: Unsupported

1072_0 (ver: 903) Voltage Ratio Input: Unsupported

1073_0 (ver: 904) Voltage Ratio Input: Unsupported

1018_3 (ver: 1000, 1001) Voltage Ratio Input: Unsupported

1046_0 (ver: 100, 101) Bridge Input: Def: BRIDGE_GAIN_128

1046_0 (ver: 102) Bridge Input: Def: BRIDGE_GAIN_128

1046_1 (ver: 200, 201) Bridge Input: Def: BRIDGE_GAIN_128

1065_0 (ver: 100, 101) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1065_1 (ver: 100, 101) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1202_0 (ver: 100) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1203_0 (ver: 100) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1202_0 (ver: 120, 121) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1202_1 (ver: 123, 124) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1203_0 (ver: 120, 121) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1203_1 (ver: 123, 124) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Def: BRIDGE_GAIN_128

1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0000_0 (ver: 117, 118, 119) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0000_0 (ver: 121, 125, 126, 127) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0000_0 (ver: 307) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0001_0 (ver: 111, 113, 114) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0001_0 (ver: 115, 116) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB5000_0 (ver: 100) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB5000_0 (ver: 102, 104, 105, 106) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB5000_0 (ver: 107) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB5000_0 (ver: 203, 204, 205) Voltage Ratio Input: Def: BRIDGE_GAIN_128

SBC3003_0 (ver: 101, 102) Voltage Ratio Input: Def: BRIDGE_GAIN_128

SBC3003_0 (ver: 108, 109, 110) Voltage Ratio Input: Def: BRIDGE_GAIN_128

SBC3003_0 (ver: 203, 204) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0000_1 (ver: 400, 401) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0002_0 (ver: 100, 101) Voltage Ratio Input: Def: BRIDGE_GAIN_128

HUB0007_0 (ver: 101, 102) Voltage Ratio Input: Def: BRIDGE_GAIN_128

DAQ1000_0 (ver: 102, 103) Voltage Ratio Input: Def: BRIDGE_GAIN_128

DAQ1000_0 (ver: 110, 111, 112, 114) Voltage Ratio Input: Def: BRIDGE_GAIN_128

DAQ1500_0 (ver: 104) Bridge Input: Def: BRIDGE_GAIN_128

DCC1000_0 (ver: 115) Voltage Ratio: Def: BRIDGE_GAIN_128

DCC1000_0 (ver: 204, 205, 206) Voltage Ratio: Def: BRIDGE_GAIN_128

DCC1000_0 (ver: 210, 211, 220) Voltage Ratio: Def: BRIDGE_GAIN_128

HIN1100_0 (ver: 104, 105, 106) Thumbstick Axis: Def: BRIDGE_GAIN_128

HUM1100_0 (ver: 100) Moisture Sensor: Def: BRIDGE_GAIN_128

HUM1100_1 (ver: 100) Moisture Sensor: Def: BRIDGE_GAIN_128

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.