## Phidget Temperature Sensor.lvlib:TemperatureSetDataInterval.vi

The `DataInterval` is the time that must elapse before the channel will fire another `TemperatureChange` event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.
- The timing between `TemperatureChange` events can also be affected by the `TemperatureChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1045_0 (ver: 100, 101) Temperature Sensor (IR): Min: 32 Max: 60000 Def: 256 1045_1 (ver: 101) Temperature Sensor (IR): Min: 32 Max: 60000 Def: 256 1045_0 (ver: 100, 101) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1045_1 (ver: 101) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_0 (ver: 100, 101, 102) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_1 (ver: 200, 202, 204, 205) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_2 (ver: 210, 212, 214, 215) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1048_1 (ver: 200, 202, 204, 205) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1048_2 (ver: 210, 212, 214, 215) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_0 (ver: 100) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 100) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Thermocouple Input: Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Min: 32 Max: 60000 Def: 256 DCC1000_0 (ver: 115) Temperature Sensor: Min: 500 Max: 60000Val: 500 DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Min: 500 Max: 60000Val: 500 DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Min: 500 Max: 60000Val: 500 DCC1100_0 (ver: 113, 114) Temperature Sensor: Min: 100 Max: 60000 Def: 250 DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Min: 100 Max: 60000 Def: 250 HUM1000_0 (ver: 104, 105) Temperature Sensor: Min: 500 Max: 60000 Def: 500 HUM1001_0 (ver: 102) Temperature Sensor: Min: 50 Max: 60000 Def: 250 MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Min: 4 Max: 60000 Def: 256 MOT0110_0 (ver: 100, 104, 110) Temperature Sensor: Min: 10 Max: 60000 Def: 250 MOT0110_0 (ver: 100, 104, 110) Temperature Sensor: Min: 10 Max: 60000 Def: 250 SAF1000_0 (ver: 101, 102) Temperature Sensor: Min: 100 Max: 60000 Def: 250 SAF1000_0 (ver: 110, 120) Temperature Sensor: Min: 100 Max: 60000 Def: 250 TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Min: 500 Max: 60000Val: 500 TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Min: 20 Max: 60000 Def: 250 TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Min: 300 Max: 60000 Def: 500 TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Min: 250 Max: 60000 Def: 250 TMP1200_1 (ver: 300, 301, 302) RTD input: Min: 333 Max: 60000 Def: 333

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.