## Phidget LCD.lvlib:LCDStart.vi

Opens and initializes a Phidget LCD

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Contrast The contrast value 1202_0 (ver: 100) Text LCD: Min: 0 Max: 1Val: 0.502 1202_0 (ver: 120, 121) Text LCD: Min: 0 Max: 1Val: 0.502 1202_1 (ver: 123, 124) Text LCD: Min: 0 Max: 1Val: 0.502 1203_0 (ver: 100) Text LCD: Min: 0 Max: 1Val: 0.502 1203_0 (ver: 120, 121) Text LCD: Min: 0 Max: 1Val: 0.502 1203_1 (ver: 123, 124) Text LCD: Min: 0 Max: 1Val: 0.502 1202_2 (ver: 200, 201, 202, 203, 204) Text LCD: Min: 0 Max: 1Val: 0.491 1203_2 (ver: 200, 201, 202, 203, 204) Text LCD: Min: 0 Max: 1Val: 0.491 1204_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0.785 1215_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0.5 1216_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0.5 1217_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0.5 1218_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0.5 1219_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0.5 1220_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0.5 1221_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0.5 1222_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0.5 LCD1100_0 (ver: 106, 107, 108, 110) Graphic LCD: Min: 0 Max: 1 Def: 0.25 LCD1100_1 (ver: 200, 201) Graphic LCD: Min: 0 Max: 1 Def: 0.25

| Backlight The backlight value 1202_0 (ver: 100) Text LCD: Min: 0 Max: 1Val: 0 1202_0 (ver: 120, 121) Text LCD: Min: 0 Max: 1Val: 0 1202_1 (ver: 123, 124) Text LCD: Min: 0 Max: 1Val: 0 1203_0 (ver: 100) Text LCD: Min: 0 Max: 1Val: 0 1203_0 (ver: 120, 121) Text LCD: Min: 0 Max: 1Val: 0 1203_1 (ver: 123, 124) Text LCD: Min: 0 Max: 1Val: 0 1202_2 (ver: 200, 201, 202, 203, 204) Text LCD: Min: 0 Max: 1Val: 0 1203_2 (ver: 200, 201, 202, 203, 204) Text LCD: Min: 0 Max: 1Val: 0 1204_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0 1215_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0 1216_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0 1217_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0 1218_0 (ver: 100, 101) Text LCD: Min: 0 Max: 1Val: 0 1219_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0 1220_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0 1221_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0 1222_0 (ver: 110, 111, 113) Text LCD: Min: 0 Max: 1Val: 0 LCD1100_0 (ver: 106, 107, 108, 110) Graphic LCD: Min: 0 Max: 1Val: 0 LCD1100_1 (ver: 200, 201) Graphic LCD: Min: 0 Max: 1Val: 0

| Timeout (mSec) Timeout in milliseconds

| Screen Size The screen size
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1202_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v100 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | 1204_0 v100 v101 | 1215_0 v100 v101 | 1216_0 v100 v101 | 1217_0 v100 v101 | 1218_0 v100 v101 | 1219_0 v110 v111 v113 | 1220_0 v110 v111 v113 | 1221_0 v110 v111 v113 | 1222_0 v110 v111 v113 | LCD1100_0 v106 v107 v108 v110 | LCD1100_1 v200 v201
SCREEN_SIZE_NONE | 1 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_64x128 | 13 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
SCREEN_SIZE_2x8 | 3 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_1x16 | 4 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x16 | 5 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_4x16 | 6 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_1x8 | 2 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_4x20 | 8 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x24 | 9 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_1x40 | 10 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x40 | 11 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_4x40 | 12 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x20 | 7 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | X

1202_0 (ver: 100) Text LCD: Val: SCREEN_SIZE_2x20

1202_0 (ver: 120, 121) Text LCD: Val: SCREEN_SIZE_2x20

1202_1 (ver: 123, 124) Text LCD: Val: SCREEN_SIZE_2x20

1203_0 (ver: 100) Text LCD: Val: SCREEN_SIZE_2x20

1203_0 (ver: 120, 121) Text LCD: Val: SCREEN_SIZE_2x20

1203_1 (ver: 123, 124) Text LCD: Val: SCREEN_SIZE_2x20

1202_2 (ver: 200, 201, 202, 203, 204) Text LCD: Val: SCREEN_SIZE_2x20

1203_2 (ver: 200, 201, 202, 203, 204) Text LCD: Val: SCREEN_SIZE_2x20

1204_0 (ver: 100, 101) Text LCD:

1215_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20

1216_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20

1217_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20

1218_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20

1219_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20

1220_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20

1221_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20

1222_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20

LCD1100_0 (ver: 106, 107, 108, 110) Graphic LCD: Val: SCREEN_SIZE_64x128

LCD1100_1 (ver: 200, 201) Graphic LCD: Val: SCREEN_SIZE_64x128

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number