## Phidget DC Motor.lvlib:DCMotorSetCurrentLimit.vi

The controller will limit the current through the motor to the `CurrentLimit` value.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Current Limit The current limit value Units: amperes (A) 1060_0 (ver: 100, 110) DC Motor Controller: Unsupported 1064_0 (ver: 100, 101, 102) DC Motor Controller: Unsupported 1064_1 (ver: 102) DC Motor Controller: Unsupported 1065_0 (ver: 100, 101) DC Motor Controller: Unsupported 1065_1 (ver: 100, 101) DC Motor Controller: Unsupported DCC1000_0 (ver: 115) DC Motor Controller: Min: 2 Max: 25Val: 2 DCC1000_0 (ver: 204, 205, 206) DC Motor Controller: Min: 2 Max: 25Val: 2 DCC1000_0 (ver: 210, 211, 220) DC Motor Controller: Min: 2 Max: 25Val: 2 DCC1001_0 (ver: 114, 116, 117) DC Motor Controller: Min: 0 Max: 2 Def: 2 DCC1001_0 (ver: 120, 130) DC Motor Controller: Min: 0 Max: 2 Def: 2 DCC1002_0 (ver: 100, 101, 102) DC Motor Controller: Min: 0 Max: 4 Def: 2 DCC1002_0 (ver: 111, 120) DC Motor Controller: Min: 0 Max: 4 Def: 2 DCC1003_0 (ver: 100, 101, 102) DC Motor Controller: Min: 0 Max: 4 Def: 2 DCC1003_0 (ver: 110, 120) DC Motor Controller: Min: 0 Max: 4 Def: 2

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.