## Phidget Voltage Input.lvlib:VoltageInputSetVoltageTrigger.vi

The channel will not issue a `VoltageChange` event until the voltage value has changed by the amount specified by the `VoltageChangeTrigger`.

- Setting the `VoltageChangeTrigger` to 0 will result in the channel firing events every `DataInterval`. This is useful for applications that implement their own data filtering

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Trigger The change trigger value Units: volts (V) 1011_0 (ver: 100, 101, 102, 103) Voltage Input: Min: 0 Max: 5 Def: 0 1013_0 (ver: 800, 811, 820) Voltage Input: Min: 0 Max: 5 Def: 0 1013_0 (ver: 821, 823) Voltage Input: Min: 0 Max: 5 Def: 0 1018_0 (ver: 824, 825, 826) Voltage Input: Min: 0 Max: 5 Def: 0 1018_1 (ver: 826) Voltage Input: Min: 0 Max: 5 Def: 0 1019_0 (ver: 826) Voltage Input: Min: 0 Max: 5 Def: 0 1070_0 (ver: 826) Voltage Input: Min: 0 Max: 5 Def: 0 1010_0 (ver: 903, 904) Voltage Input: Min: 0 Max: 5 Def: 0 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: Min: 0 Max: 5 Def: 0 1019_1 (ver: 903, 904) Voltage Input: Min: 0 Max: 5 Def: 0 1072_0 (ver: 903) Voltage Input: Min: 0 Max: 5 Def: 0 1073_0 (ver: 904) Voltage Input: Min: 0 Max: 5 Def: 0 1018_3 (ver: 1000, 1001) Voltage Input: Min: 0 Max: 5 Def: 0 1048_0 (ver: 100, 101, 102) Voltage Input: Min: 0 Max: 0.08742 Def: 0 1048_1 (ver: 200, 202, 204, 205) Voltage Input: Min: 0 Max: 0.08742 Def: 0 1048_2 (ver: 210, 212, 214, 215) Voltage Input: Min: 0 Max: 0.08742 Def: 0 1051_0 (ver: 200, 201, 202) Voltage Input: Min: 0 Max: 0.08742 Def: 0 1051_1 (ver: 300) Voltage Input: Min: 0 Max: 0.08742 Def: 0 1051_2 (ver: 400, 401, 402) Voltage Input: Min: 0 Max: 0.08742 Def: 0 1058_0 (ver: 100, 101) Voltage Input: Min: 0 Max: 0.1054 Def: 0 1065_0 (ver: 100, 101) Voltage Input: Min: 0 Max: 5 Def: 0 1065_1 (ver: 100, 101) Voltage Input: Min: 0 Max: 5 Def: 0 1065_0 (ver: 100, 101) Supply Voltage Sensor: Min: 0 Max: 80 Def: 0 1065_1 (ver: 100, 101) Supply Voltage Sensor: Min: 0 Max: 80 Def: 0 1202_0 (ver: 100) Voltage Input: Min: 0 Max: 5 Def: 0 1203_0 (ver: 100) Voltage Input: Min: 0 Max: 5 Def: 0 1202_0 (ver: 120, 121) Voltage Input: Min: 0 Max: 5 Def: 0 1202_1 (ver: 123, 124) Voltage Input: Min: 0 Max: 5 Def: 0 1203_0 (ver: 120, 121) Voltage Input: Min: 0 Max: 5 Def: 0 1203_1 (ver: 123, 124) Voltage Input: Min: 0 Max: 5 Def: 0 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Min: 0 Max: 5 Def: 0 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0000_0 (ver: 117, 118, 119) Voltage Input: Min: 0 Max: 5 Def: 0 HUB5000_0 (ver: 100) Voltage Input: Min: 0 Max: 5 Def: 0 SBC3003_0 (ver: 101, 102) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0000_0 (ver: 121, 125, 126, 127) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0000_0 (ver: 307) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0001_0 (ver: 111, 113, 114) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0001_0 (ver: 115, 116) Voltage Input: Min: 0 Max: 5 Def: 0 HUB5000_0 (ver: 102, 104, 105, 106) Voltage Input: Min: 0 Max: 5 Def: 0 HUB5000_0 (ver: 107) Voltage Input: Min: 0 Max: 5 Def: 0 HUB5000_0 (ver: 203, 204, 205) Voltage Input: Min: 0 Max: 5 Def: 0 SBC3003_0 (ver: 108, 109, 110) Voltage Input: Min: 0 Max: 5 Def: 0 SBC3003_0 (ver: 203, 204) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0000_1 (ver: 400, 401) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0002_0 (ver: 100, 101) Voltage Input: Min: 0 Max: 5 Def: 0 HUB0007_0 (ver: 101, 102) Voltage Input: Min: 0 Max: 5 Def: 0 ADP1000_0 (ver: 104, 105) Voltage Input: Min: 0 Max: 4 Def: 0 DAQ1000_0 (ver: 102, 103) Voltage Input: Min: 0 Max: 5 Def: 0 DAQ1000_0 (ver: 110, 111, 112, 114) Voltage Input: Min: 0 Max: 5 Def: 0 DAQ1400_0 (ver: 112) Voltage Input: Min: 0 Max: 5 Def: 0 DAQ1400_0 (ver: 120, 121) Voltage Input: Min: 0 Max: 5 Def: 0 SAF1000_0 (ver: 101, 102) Voltage Sensor: Min: 0 Max: 32 Def: 0 SAF1000_0 (ver: 110, 120) Voltage Sensor: Min: 0 Max: 32 Def: 0 STC1003_1 (ver: 201, 221) Voltage Input: Min: 0 Max: 20 Def: 0 STC1005_0 (ver: 100, 110) Voltage Input: Min: 0 Max: 20 Def: 0 TMP1100_0 (ver: 103, 105, 106, 108, 109) Voltage Input: Min: 0 Max: 0.09 Def: 0 TMP1101_0 (ver: 104, 106, 107, 109) Voltage Input: Min: 0 Max: 0.09 Def: 0 TMP1101_1 (ver: 201, 202, 203) Voltage Input: Min: 0 Max: 0.09 Def: 0 VCP1000_0 (ver: 100, 101) Voltage Input: Min: 0 Max: 80 Def: 0 VCP1001_0 (ver: 100) Voltage Input: Min: 0 Max: 80 Def: 0 VCP1001_0 (ver: 110) Voltage Input: Min: 0 Max: 80 Def: 0 VCP1002_0 (ver: 106) Voltage Input: Min: 0 Max: 2 Def: 0 VCP1002_0 (ver: 110) Voltage Input: Min: 0 Max: 2 Def: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.