## Phidget Temperature Sensor.lvlib:TemperatureSetThermocoupleType.vi

The `ThermocoupleType` must correspond to the thermocouple type you are using in your application.

- If you are unsure which `ThermocoupleType` to use, visit the Thermocouple Primer for more information.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| ThermocoupleType The thermocouple type
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1045_0 v100 v101 | 1045_1 v101 | 1045_0 v100 v101 | 1045_1 v101 | 1048_0 v100 v101 v102 | 1048_0 v100 v101 v102 | 1048_1 v200 v202 v204 v205 | 1048_2 v210 v212 v214 v215 | 1048_1 v200 v202 v204 v205 | 1048_2 v210 v212 v214 v215 | 1051_0 v100 | 1051_0 v100 | 1051_0 v200 v201 v202 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_1 v300 | 1051_2 v400 v401 v402 | 1051_2 v400 v401 v402 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220 | DCC1100_0 v113 v114 | DCC1100_0 v120 v121 v130 | HUM1000_0 v104 v105 | HUM1001_0 v102 | MOT0109_0 v112 v113 v115 v117 | MOT0110_0 v100 v104 v110 | MOT0110_0 v100 v104 v110 | SAF1000_0 v101 v102 | SAF1000_0 v110 v120 | TMP1000_0 v105 v107 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1100_0 v103 v105 v106 v108 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_1 v201 v202 v203 | TMP1101_1 v201 v202 v203 | TMP1200_0 v104 v105 v106 v107 v108 v109 v110 | TMP1200_1 v300 v301 v302
THERMOCOUPLE_TYPE_J | 1 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X
THERMOCOUPLE_TYPE_K | 2 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | ✓ | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X
THERMOCOUPLE_TYPE_E | 3 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X
THERMOCOUPLE_TYPE_T | 4 | X | X | X | X | ✓ | X | ✓ | ✓ | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | ✓ | X | ✓ | X | X | X
1045_0 (ver: 100, 101) Temperature Sensor (IR): Unsupported 1045_1 (ver: 101) Temperature Sensor (IR): Unsupported 1045_0 (ver: 100, 101) Temperature Sensor (IC): Unsupported 1045_1 (ver: 101) Temperature Sensor (IC): Unsupported 1048_0 (ver: 100, 101, 102) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1048_1 (ver: 200, 202, 204, 205) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_2 (ver: 210, 212, 214, 215) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_1 (ver: 200, 202, 204, 205) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1048_2 (ver: 210, 212, 214, 215) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1051_0 (ver: 100) Thermocouple Input: Val: THERMOCOUPLE_TYPE_K 1051_0 (ver: 100) Temperature Sensor (IC): Val: THERMOCOUPLE_TYPE_K 1051_0 (ver: 200, 201, 202) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1051_1 (ver: 300) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_1 (ver: 300) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K 1051_2 (ver: 400, 401, 402) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K DCC1000_0 (ver: 115) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1000_0 (ver: 210, 211, 220) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1100_0 (ver: 113, 114) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K DCC1100_0 (ver: 120, 121, 130) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K HUM1000_0 (ver: 104, 105) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K HUM1001_0 (ver: 102) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K MOT0110_0 (ver: 100, 104, 110) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K MOT0110_0 (ver: 100, 104, 110) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K SAF1000_0 (ver: 101, 102) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K SAF1000_0 (ver: 110, 120) Temperature Sensor: Def: THERMOCOUPLE_TYPE_K TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1100_0 (ver: 103, 105, 106, 108, 109) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1100_0 (ver: 103, 105, 106, 108, 109) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1101_0 (ver: 104, 106, 107, 109) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1101_0 (ver: 104, 106, 107, 109) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1101_1 (ver: 201, 202, 203) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1101_1 (ver: 201, 202, 203) Temperature Sensor (IC): Def: THERMOCOUPLE_TYPE_K TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input: Def: THERMOCOUPLE_TYPE_K TMP1200_1 (ver: 300, 301, 302) RTD input: Def: THERMOCOUPLE_TYPE_K

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.