## Phidget Current Input.lvlib:CurrentInputSetPowerSupply.vi

Choose the power supply voltage.

- Set this to the voltage specified in the attached sensor's data sheet to power it.

- Set to `POWER_SUPPLY_OFF` to turn off the supply to save power.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Power Supply The power supply value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1061_0 v100 | 1061_0 v200 | 1061_1 v300 v301 v302 v303 v304 | 1063_0 v100 | 1063_1 v100 v101 | 1064_0 v100 v101 v102 | 1064_1 v102 | 1065_0 v100 v101 | 1065_1 v100 v101 | 1066_0 v100 | 1066_1 v100 v101 | DAQ1400_0 v112 | DAQ1400_0 v120 v121 | VCP1100_0 v101 v102 | DCC1000_0 v115 | DCC1000_0 v204 v205 v206 | DCC1000_0 v210 v211 v220
POWER_SUPPLY_OFF | 1 | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X | X | X
POWER_SUPPLY_12V | 2 | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X | X | X
POWER_SUPPLY_24V | 3 | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X | X | X
1061_0 (ver: 100) RC Servo Motor Current Sensor: Unsupported 1061_0 (ver: 200) RC Servo Motor Current Sensor: Unsupported 1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Current Sensor: Unsupported 1063_0 (ver: 100) Bipolar Stepper Current Sensor: Unsupported 1063_1 (ver: 100, 101) Bipolar Stepper Current Sensor: Unsupported 1064_0 (ver: 100, 101, 102) DC Motor Current Sensor: Unsupported 1064_1 (ver: 102) DC Motor Current Sensor: Unsupported 1065_0 (ver: 100, 101) DC Motor Current Sensor: Unsupported 1065_1 (ver: 100, 101) DC Motor Current Sensor: Unsupported 1066_0 (ver: 100) RC Servo Motor Current Sensor: Unsupported 1066_1 (ver: 100, 101) RC Servo Motor Current Sensor: Unsupported DAQ1400_0 (ver: 112) Current Input: Def: POWER_SUPPLY_12V DAQ1400_0 (ver: 120, 121) Current Input: Def: POWER_SUPPLY_12V VCP1100_0 (ver: 101, 102) Current Input: Def: POWER_SUPPLY_12V DCC1000_0 (ver: 115) Current Sensor: Def: POWER_SUPPLY_12V DCC1000_0 (ver: 204, 205, 206) Current Sensor: Def: POWER_SUPPLY_12V DCC1000_0 (ver: 210, 211, 220) Current Sensor: Def: POWER_SUPPLY_12V

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.