## Phidget Voltage Input.lvlib:VoltageInputSetVoltageRange.vi

The voltage range you choose should allow you to measure the full range of your input signal.

- A larger `VoltageRange` equates to less resolution.
- If a `Saturation` event occurs, increase the voltage range.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Voltage Range The voltage range value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1011_0 v100 v101 v102 v103 | 1013_0 v800 v811 v820 | 1013_0 v821 v823 | 1018_0 v824 v825 v826 | 1018_1 v826 | 1019_0 v826 | 1070_0 v826 | 1010_0 v903 v904 | 1018_2 v900 v901 v902 v903 v904 | 1019_1 v903 v904 | 1072_0 v903 | 1073_0 v904 | 1018_3 v1000 v1001 | 1048_0 v100 v101 v102 | 1048_1 v200 v202 v204 v205 | 1048_2 v210 v212 v214 v215 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_2 v400 v401 v402 | 1058_0 v100 v101 | 1065_0 v100 v101 | 1065_1 v100 v101 | 1065_0 v100 v101 | 1065_1 v100 v101 | 1202_0 v100 | 1203_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | HUB0000_0 v117 v118 v119 | HUB5000_0 v100 | SBC3003_0 v101 v102 | HUB0000_0 v121 v125 v126 v127 | HUB0000_0 v307 | HUB0001_0 v111 v113 v114 | HUB0001_0 v115 v116 | HUB5000_0 v102 v104 v105 v106 | HUB5000_0 v107 | HUB5000_0 v203 v204 v205 | SBC3003_0 v108 v109 v110 | SBC3003_0 v203 v204 | HUB0000_1 v400 v401 | HUB0002_0 v100 v101 | HUB0007_0 v101 v102 | ADP1000_0 v104 v105 | DAQ1000_0 v102 v103 | DAQ1000_0 v110 v111 v112 v114 | DAQ1400_0 v112 | DAQ1400_0 v120 v121 | SAF1000_0 v101 v102 | SAF1000_0 v110 v120 | STC1003_1 v201 v221 | STC1005_0 v100 v110
| TMP1100_0 v103 v105 v106 v108 v109 | TMP1101_0 v104 v106 v107 v109 | TMP1101_1 v201 v202 v203 | VCP1000_0 v100 v101 | VCP1001_0 v100 | VCP1001_0 v110 | VCP1002_0 v106 | VCP1002_0 v110
VOLTAGE_RANGE_10mV | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_AUTO | 11 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | ✓
VOLTAGE_RANGE_200mV | 3 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_312_5mV | 4 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X
VOLTAGE_RANGE_400mV | 5 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X
VOLTAGE_RANGE_40mV | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_2V | 7 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X
VOLTAGE_RANGE_5V | 8 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X
VOLTAGE_RANGE_15V | 9 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | X | X
VOLTAGE_RANGE_40V | 10 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | X | X
VOLTAGE_RANGE_1000mV | 6 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓

1011_0 (ver: 100, 101, 102, 103) Voltage Input: Unsupported

1013_0 (ver: 800, 811, 820) Voltage Input: Unsupported

1013_0 (ver: 821, 823) Voltage Input: Unsupported

1018_0 (ver: 824, 825, 826) Voltage Input: Unsupported

1018_1 (ver: 826) Voltage Input: Unsupported

1019_0 (ver: 826) Voltage Input: Unsupported

1070_0 (ver: 826) Voltage Input: Unsupported

1010_0 (ver: 903, 904) Voltage Input: Unsupported

1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: Unsupported

1019_1 (ver: 903, 904) Voltage Input: Unsupported

1072_0 (ver: 903) Voltage Input: Unsupported

1073_0 (ver: 904) Voltage Input: Unsupported

1018_3 (ver: 1000, 1001) Voltage Input: Unsupported

1048_0 (ver: 100, 101, 102) Voltage Input: Unsupported

1048_1 (ver: 200, 202, 204, 205) Voltage Input: Unsupported

1048_2 (ver: 210, 212, 214, 215) Voltage Input: Unsupported

1051_0 (ver: 200, 201, 202) Voltage Input: Unsupported

1051_1 (ver: 300) Voltage Input: Unsupported

1051_2 (ver: 400, 401, 402) Voltage Input: Unsupported

1058_0 (ver: 100, 101) Voltage Input: Unsupported

1065_0 (ver: 100, 101) Voltage Input: Unsupported

1065_1 (ver: 100, 101) Voltage Input: Unsupported

1065_0 (ver: 100, 101) Supply Voltage Sensor: Unsupported

1065_1 (ver: 100, 101) Supply Voltage Sensor: Unsupported

1202_0 (ver: 100) Voltage Input: Unsupported

1203_0 (ver: 100) Voltage Input: Unsupported

1202_0 (ver: 120, 121) Voltage Input: Unsupported

1202_1 (ver: 123, 124) Voltage Input: Unsupported

1203_0 (ver: 120, 121) Voltage Input: Unsupported

1203_1 (ver: 123, 124) Voltage Input: Unsupported

1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Unsupported

1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Unsupported

HUB0000_0 (ver: 117, 118, 119) Voltage Input: Unsupported

HUB5000_0 (ver: 100) Voltage Input: Unsupported

SBC3003_0 (ver: 101, 102) Voltage Input: Unsupported

HUB0000_0 (ver: 121, 125, 126, 127) Voltage Input: Unsupported

HUB0000_0 (ver: 307) Voltage Input: Unsupported

HUB0001_0 (ver: 111, 113, 114) Voltage Input: Unsupported

HUB0001_0 (ver: 115, 116) Voltage Input: Unsupported

HUB5000_0 (ver: 102, 104, 105, 106) Voltage Input: Unsupported

HUB5000_0 (ver: 107) Voltage Input: Unsupported

HUB5000_0 (ver: 203, 204, 205) Voltage Input: Unsupported

SBC3003_0 (ver: 108, 109, 110) Voltage Input: Unsupported

SBC3003_0 (ver: 203, 204) Voltage Input: Unsupported

HUB0000_1 (ver: 400, 401) Voltage Input: Unsupported

HUB0002_0 (ver: 100, 101) Voltage Input: Unsupported

HUB0007_0 (ver: 101, 102) Voltage Input: Unsupported

ADP1000_0 (ver: 104, 105) Voltage Input: Def: VOLTAGE_RANGE_400mV

DAQ1000_0 (ver: 102, 103) Voltage Input: Def: VOLTAGE_RANGE_400mV

DAQ1000_0 (ver: 110, 111, 112, 114) Voltage Input: Def: VOLTAGE_RANGE_400mV

DAQ1400_0 (ver: 112) Voltage Input: Def: VOLTAGE_RANGE_400mV

DAQ1400_0 (ver: 120, 121) Voltage Input: Def: VOLTAGE_RANGE_400mV

SAF1000_0 (ver: 101, 102) Voltage Sensor: Def: VOLTAGE_RANGE_400mV

SAF1000_0 (ver: 110, 120) Voltage Sensor: Def: VOLTAGE_RANGE_400mV

STC1003_1 (ver: 201, 221) Voltage Input: Def: VOLTAGE_RANGE_400mV

STC1005_0 (ver: 100, 110) Voltage Input: Def: VOLTAGE_RANGE_400mV

TMP1100_0 (ver: 103, 105, 106, 108, 109) Voltage Input: Def: VOLTAGE_RANGE_400mV

TMP1101_0 (ver: 104, 106, 107, 109) Voltage Input: Def: VOLTAGE_RANGE_400mV

TMP1101_1 (ver: 201, 202, 203) Voltage Input: Def: VOLTAGE_RANGE_400mV

VCP1000_0 (ver: 100, 101) Voltage Input: Def: VOLTAGE_RANGE_40V

VCP1001_0 (ver: 100) Voltage Input: Def: VOLTAGE_RANGE_AUTO

VCP1001_0 (ver: 110) Voltage Input: Def: VOLTAGE_RANGE_AUTO

VCP1002_0 (ver: 106) Voltage Input: Def: VOLTAGE_RANGE_AUTO

VCP1002_0 (ver: 110) Voltage Input: Def: VOLTAGE_RANGE_AUTO

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.