## Phidget Resistance Input.lvlib:ResistanceInputStart.vi

Opens and initializes a Phidget Resistance Input

| Change Trigger The change trigger value Units: ohms (Ω) TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) Resistance Input: Min: 0 Max: 19000 Def: 0 TMP1200_1 (ver: 300, 301, 302) Resistance Input: Min: 0 Max: 5000 Def: 0

| Data Interval The data interval value Units: milliseconds (ms) TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) Resistance Input: Min: 250 Max: 60000 Def: 250 TMP1200_1 (ver: 300, 301, 302) Resistance Input: Min: 333 Max: 60000 Def: 333

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| RTD Wire Setup Wire setup value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
TMP1200_0 v104 v105 v106 v107 v108 v109 v110 | TMP1200_1 v300 v301 v302
RTD_WIRE_SETUP_2WIRE | 1 | ✓ | ✓
RTD_WIRE_SETUP_3WIRE | 2 | ✓ | ✓
RTD_WIRE_SETUP_4WIRE | 3 | ✓ | ✓

TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) Resistance Input: Def: RTD_WIRE_SETUP_4WIRE

TMP1200_1 (ver: 300, 301, 302) Resistance Input: Def: RTD_WIRE_SETUP_4WIRE

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number