## Phidget Gyroscope.lvlib:GyroscopeEventExe.vi

The most recent angular rate and timestamp values the channel has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

Device Support:

1042_0 (ver: 300, 301, 302, 303) 3-Axis Gyroscope : Supported

1044_0 (ver: 400, 401, 402, 403) 3-Axis Gyroscope : Supported

1044_1 (ver: 500, 502) 3-Axis Gyroscope : Supported

1044_1 (ver: 511) 3-Axis Gyroscope : Supported

1056_0 (ver: 100, 101, 102) 3-Axis Gyroscope : Supported

1056_0 (ver: 200) 3-Axis Gyroscope : Supported

MOT1101_0 (ver: 112, 113) 3-Axis Gyroscope : Supported

MOT1102_0 (ver: 210, 212) 3-Axis Gyroscope : Supported

MOT1102_1 (ver: 300, 301) 3-Axis Gyroscope : Supported

MOT0109_0 (ver: 112, 113, 115, 117) 3-Axis Gyroscope : Supported

MOT0110_0 (ver: 100, 104, 110) 3-Axis Gyroscope : Supported

MOT0110_0 (ver: 100, 104, 110) 3-Axis Gyroscope : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| phid Device # Identification of the device that triggered the event.

| Timestamp The timestamp value

| Angular Rate The angular rate values

| Angular Rate Angular Rate

| Event Registration Refnum Out Same as Event Registration Refnum In