## Phidget Data Adapter.lvlib:DataAdapterSetFrequency.vi

The rate at which data is transmitted over the communication lines in bits per second.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Frequency The communication frequency to use for future data transfers. Units: bits per second (bps)
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
ADP0001_0 v200 | ADP0001_0 v200 | ADP0002_0 v100 | ADP0002_0 v100
FREQUENCY_10kHz | 1 | ✓ | ✓ | X | X
FREQUENCY_100kHz | 2 | ✓ | ✓ | X | X
FREQUENCY_400kHz | 3 | ✓ | ✓ | X | X
FREQUENCY_188kHz | 4 | X | X | ✓ | ✓
FREQUENCY_375kHz | 5 | X | X | ✓ | ✓
FREQUENCY_750kHz | 6 | X | X | ✓ | ✓
FREQUENCY_1500kHz | 7 | X | X | ✓ | ✓
FREQUENCY_3MHz | 8 | X | X | ✓ | ✓
FREQUENCY_6MHz | 9 | X | X | ✓ | ✓
ADP0001_0 (ver: 200) Data Adapter: Default: FREQUENCY_100kHz ADP0001_0 (ver: 200) Data Adapter: Default: FREQUENCY_100kHz ADP0002_0 (ver: 100) Data Adapter: Default: FREQUENCY_1500kHz ADP0002_0 (ver: 100) Data Adapter: Default: FREQUENCY_1500kHz

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.